Fitter report for myArkanoid
Mon May 28 14:22:25 2012
Quartus II Version 9.1 Build 222 10/21/2009 SJ Full Version


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Fitter Summary
  3. Fitter Settings
  4. Parallel Compilation
  5. Incremental Compilation Preservation Summary
  6. Incremental Compilation Partition Settings
  7. Incremental Compilation Placement Preservation
  8. Pin-Out File
  9. Fitter Resource Usage Summary
 10. Input Pins
 11. Output Pins
 12. I/O Bank Usage
 13. All Package Pins
 14. Output Pin Default Load For Reported TCO
 15. Fitter Resource Utilization by Entity
 16. Delay Chain Summary
 17. Pad To Core Delay Chain Fanout
 18. Control Signals
 19. Global & Other Fast Signals
 20. Non-Global High Fan-Out Signals
 21. Interconnect Usage Summary
 22. LAB Logic Elements
 23. LAB-wide Signals
 24. LAB Signals Sourced
 25. LAB Signals Sourced Out
 26. LAB Distinct Inputs
 27. Fitter Device Options
 28. Operating Settings and Conditions
 29. Estimated Delay Added for Hold Timing
 30. Fitter Messages
 31. Fitter Suppressed Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.



+-------------------------------------------------------------------------------+
; Fitter Summary                                                                ;
+------------------------------------+------------------------------------------+
; Fitter Status                      ; Successful - Mon May 28 14:22:24 2012    ;
; Quartus II Version                 ; 9.1 Build 222 10/21/2009 SJ Full Version ;
; Revision Name                      ; myArkanoid                               ;
; Top-level Entity Name              ; TotalScheme                              ;
; Family                             ; Cyclone II                               ;
; Device                             ; EP2C20F484C7                             ;
; Timing Models                      ; Final                                    ;
; Total logic elements               ; 7,148 / 18,752 ( 38 % )                  ;
;     Total combinational functions  ; 7,096 / 18,752 ( 38 % )                  ;
;     Dedicated logic registers      ; 1,086 / 18,752 ( 6 % )                   ;
; Total registers                    ; 1086                                     ;
; Total pins                         ; 55 / 315 ( 17 % )                        ;
; Total virtual pins                 ; 0                                        ;
; Total memory bits                  ; 0 / 239,616 ( 0 % )                      ;
; Embedded Multiplier 9-bit elements ; 0 / 52 ( 0 % )                           ;
; Total PLLs                         ; 0 / 4 ( 0 % )                            ;
+------------------------------------+------------------------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Settings                                                                                                                              ;
+----------------------------------------------------------------------------+--------------------------------+--------------------------------+
; Option                                                                     ; Setting                        ; Default Value                  ;
+----------------------------------------------------------------------------+--------------------------------+--------------------------------+
; Device                                                                     ; EP2C20F484C7                   ;                                ;
; Minimum Core Junction Temperature                                          ; 0                              ;                                ;
; Maximum Core Junction Temperature                                          ; 85                             ;                                ;
; Fit Attempts to Skip                                                       ; 0                              ; 0.0                            ;
; Use smart compilation                                                      ; Off                            ; Off                            ;
; Enable parallel Assembler and TimeQuest Timing Analyzer during compilation ; On                             ; On                             ;
; Enable compact report table                                                ; Off                            ; Off                            ;
; Use TimeQuest Timing Analyzer                                              ; Off                            ; Off                            ;
; Router Timing Optimization Level                                           ; Normal                         ; Normal                         ;
; Placement Effort Multiplier                                                ; 1.0                            ; 1.0                            ;
; Router Effort Multiplier                                                   ; 1.0                            ; 1.0                            ;
; Always Enable Input Buffers                                                ; Off                            ; Off                            ;
; Optimize Hold Timing                                                       ; IO Paths and Minimum TPD Paths ; IO Paths and Minimum TPD Paths ;
; Optimize Multi-Corner Timing                                               ; Off                            ; Off                            ;
; PowerPlay Power Optimization                                               ; Normal compilation             ; Normal compilation             ;
; Optimize Timing                                                            ; Normal compilation             ; Normal compilation             ;
; Optimize Timing for ECOs                                                   ; Off                            ; Off                            ;
; Regenerate full fit report during ECO compiles                             ; Off                            ; Off                            ;
; Optimize IOC Register Placement for Timing                                 ; On                             ; On                             ;
; Limit to One Fitting Attempt                                               ; Off                            ; Off                            ;
; Final Placement Optimizations                                              ; Automatically                  ; Automatically                  ;
; Fitter Aggressive Routability Optimizations                                ; Automatically                  ; Automatically                  ;
; Fitter Initial Placement Seed                                              ; 1                              ; 1                              ;
; PCI I/O                                                                    ; Off                            ; Off                            ;
; Weak Pull-Up Resistor                                                      ; Off                            ; Off                            ;
; Enable Bus-Hold Circuitry                                                  ; Off                            ; Off                            ;
; Auto Global Memory Control Signals                                         ; Off                            ; Off                            ;
; Auto Packed Registers                                                      ; Auto                           ; Auto                           ;
; Auto Delay Chains                                                          ; On                             ; On                             ;
; Auto Merge PLLs                                                            ; On                             ; On                             ;
; Ignore PLL Mode When Merging PLLs                                          ; Off                            ; Off                            ;
; Perform Physical Synthesis for Combinational Logic for Fitting             ; Off                            ; Off                            ;
; Perform Physical Synthesis for Combinational Logic for Performance         ; Off                            ; Off                            ;
; Perform Register Duplication for Performance                               ; Off                            ; Off                            ;
; Perform Logic to Memory Mapping for Fitting                                ; Off                            ; Off                            ;
; Perform Register Retiming for Performance                                  ; Off                            ; Off                            ;
; Perform Asynchronous Signal Pipelining                                     ; Off                            ; Off                            ;
; Fitter Effort                                                              ; Auto Fit                       ; Auto Fit                       ;
; Physical Synthesis Effort Level                                            ; Normal                         ; Normal                         ;
; Auto Global Clock                                                          ; On                             ; On                             ;
; Auto Global Register Control Signals                                       ; On                             ; On                             ;
; Stop After Congestion Map Generation                                       ; Off                            ; Off                            ;
; Save Intermediate Fitting Results                                          ; Off                            ; Off                            ;
; Force Fitter to Avoid Periphery Placement Warnings                         ; Off                            ; Off                            ;
; Use Best Effort Settings for Compilation                                   ; Off                            ; Off                            ;
+----------------------------------------------------------------------------+--------------------------------+--------------------------------+


+------------------------------------------+
; Parallel Compilation                     ;
+----------------------------+-------------+
; Processors                 ; Number      ;
+----------------------------+-------------+
; Number detected on machine ; 2           ;
; Maximum allowed            ; 2           ;
;                            ;             ;
; Average used               ; 1.20        ;
; Maximum used               ; 2           ;
;                            ;             ;
; Usage by Processor         ; % Time Used ;
;     1 processor            ; 100.0%      ;
;     2 processors           ;  11.1%      ;
+----------------------------+-------------+


+-----------------------------------------------+
; Incremental Compilation Preservation Summary  ;
+-------------------------+---------------------+
; Type                    ; Value               ;
+-------------------------+---------------------+
; Placement               ;                     ;
;     -- Requested        ; 0 / 8242 ( 0.00 % ) ;
;     -- Achieved         ; 0 / 8242 ( 0.00 % ) ;
;                         ;                     ;
; Routing (by Connection) ;                     ;
;     -- Requested        ; 0 / 0 ( 0.00 % )    ;
;     -- Achieved         ; 0 / 0 ( 0.00 % )    ;
+-------------------------+---------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------+
; Incremental Compilation Partition Settings                                                                                                       ;
+----------------+----------------+-------------------+-------------------------+------------------------+------------------------------+----------+
; Partition Name ; Partition Type ; Netlist Type Used ; Preservation Level Used ; Netlist Type Requested ; Preservation Level Requested ; Contents ;
+----------------+----------------+-------------------+-------------------------+------------------------+------------------------------+----------+
; Top            ; User-created   ; Source File       ; N/A                     ; Source File            ; N/A                          ;          ;
+----------------+----------------+-------------------+-------------------------+------------------------+------------------------------+----------+


+--------------------------------------------------------------------------------------------+
; Incremental Compilation Placement Preservation                                             ;
+----------------+---------+-------------------+-------------------------+-------------------+
; Partition Name ; # Nodes ; # Preserved Nodes ; Preservation Level Used ; Netlist Type Used ;
+----------------+---------+-------------------+-------------------------+-------------------+
; Top            ; 8242    ; 0                 ; N/A                     ; Source File       ;
+----------------+---------+-------------------+-------------------------+-------------------+


+--------------+
; Pin-Out File ;
+--------------+
The pin-out file can be found in G:/Verilog/Arkanoid2PDE1/myArkanoid.pin.


+-------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Usage Summary                                                                                                                   ;
+---------------------------------------------+---------------------------------------------------------------------------------------------------+
; Resource                                    ; Usage                                                                                             ;
+---------------------------------------------+---------------------------------------------------------------------------------------------------+
; Total logic elements                        ; 7,148 / 18,752 ( 38 % )                                                                           ;
;     -- Combinational with no register       ; 6062                                                                                              ;
;     -- Register only                        ; 52                                                                                                ;
;     -- Combinational with a register        ; 1034                                                                                              ;
;                                             ;                                                                                                   ;
; Logic element usage by number of LUT inputs ;                                                                                                   ;
;     -- 4 input functions                    ; 2860                                                                                              ;
;     -- 3 input functions                    ; 2246                                                                                              ;
;     -- <=2 input functions                  ; 1990                                                                                              ;
;     -- Register only                        ; 52                                                                                                ;
;                                             ;                                                                                                   ;
; Logic elements by mode                      ;                                                                                                   ;
;     -- normal mode                          ; 5409                                                                                              ;
;     -- arithmetic mode                      ; 1687                                                                                              ;
;                                             ;                                                                                                   ;
; Total registers*                            ; 1,086 / 19,649 ( 6 % )                                                                            ;
;     -- Dedicated logic registers            ; 1,086 / 18,752 ( 6 % )                                                                            ;
;     -- I/O registers                        ; 0 / 897 ( 0 % )                                                                                   ;
;                                             ;                                                                                                   ;
; Total LABs:  partially or completely used   ; 521 / 1,172 ( 44 % )                                                                              ;
; User inserted logic elements                ; 0                                                                                                 ;
; Virtual pins                                ; 0                                                                                                 ;
; I/O pins                                    ; 55 / 315 ( 17 % )                                                                                 ;
;     -- Clock pins                           ; 1 / 8 ( 13 % )                                                                                    ;
; Global signals                              ; 1                                                                                                 ;
; M4Ks                                        ; 0 / 52 ( 0 % )                                                                                    ;
; Total block memory bits                     ; 0 / 239,616 ( 0 % )                                                                               ;
; Total block memory implementation bits      ; 0 / 239,616 ( 0 % )                                                                               ;
; Embedded Multiplier 9-bit elements          ; 0 / 52 ( 0 % )                                                                                    ;
; PLLs                                        ; 0 / 4 ( 0 % )                                                                                     ;
; Global clocks                               ; 1 / 16 ( 6 % )                                                                                    ;
; JTAGs                                       ; 0 / 1 ( 0 % )                                                                                     ;
; ASMI blocks                                 ; 0 / 1 ( 0 % )                                                                                     ;
; CRC blocks                                  ; 0 / 1 ( 0 % )                                                                                     ;
; Average interconnect usage (total/H/V)      ; 15% / 15% / 16%                                                                                   ;
; Peak interconnect usage (total/H/V)         ; 31% / 31% / 31%                                                                                   ;
; Maximum fan-out node                        ; ClockDivider:inst1|clk25MHz_~clkctrl                                                              ;
; Maximum fan-out                             ; 1085                                                                                              ;
; Highest non-global fan-out signal           ; Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|quotient[1]~0 ;
; Highest non-global fan-out                  ; 197                                                                                               ;
; Total fan-out                               ; 24145                                                                                             ;
; Average fan-out                             ; 2.92                                                                                              ;
+---------------------------------------------+---------------------------------------------------------------------------------------------------+
*  Register count does not include registers inside RAM blocks or DSP blocks.



+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Input Pins                                                                                                                                                                                                                                                      ;
+-----------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+-------------+----------------------+
; Name      ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Cell number ; Combinational Fan-Out ; Registered Fan-Out ; Global ; Input Register ; Power Up High ; PCI I/O Enabled ; Bus Hold ; Weak Pull Up ; I/O Standard ; Termination ; Location assigned by ;
+-----------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+-------------+----------------------+
; button1   ; T21   ; 6        ; 50           ; 9            ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; button2   ; T22   ; 6        ; 50           ; 9            ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; button3   ; R21   ; 6        ; 50           ; 10           ; 2           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; button4   ; R22   ; 6        ; 50           ; 10           ; 1           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
; clk_50MHz ; L1    ; 2        ; 0            ; 13           ; 0           ; 1                     ; 0                  ; no     ; no             ; no            ; no              ; no       ; Off          ; 3.3-V LVTTL  ; Off         ; User                 ;
+-----------+-------+----------+--------------+--------------+-------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+-------------+----------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Output Pins                                                                                                                                                                                                                                                                                                                            ;
+----------+-------+----------+--------------+--------------+-------------+-----------------+------------------------+---------------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-------------+----------------------+------+----------------------+---------------------+
; Name     ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Cell number ; Output Register ; Output Enable Register ; Power Up High ; PCI I/O Enabled ; Open Drain ; TRI Primitive ; Bus Hold ; Weak Pull Up ; I/O Standard ; Current Strength ; Termination ; Location assigned by ; Load ; Output Enable Source ; Output Enable Group ;
+----------+-------+----------+--------------+--------------+-------------+-----------------+------------------------+---------------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-------------+----------------------+------+----------------------+---------------------+
; blue[0]  ; A9    ; 3        ; 15           ; 27           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; blue[1]  ; D11   ; 3        ; 22           ; 27           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; blue[2]  ; A10   ; 3        ; 20           ; 27           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; blue[3]  ; B10   ; 3        ; 20           ; 27           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; green[0] ; B8    ; 3        ; 13           ; 27           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; green[1] ; C10   ; 3        ; 18           ; 27           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; green[2] ; B9    ; 3        ; 15           ; 27           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; green[3] ; A8    ; 3        ; 13           ; 27           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; h_sync   ; A11   ; 3        ; 22           ; 27           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[0]  ; J2    ; 2        ; 0            ; 18           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[1]  ; J1    ; 2        ; 0            ; 18           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[2]  ; H2    ; 2        ; 0            ; 19           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[3]  ; H1    ; 2        ; 0            ; 19           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[4]  ; F2    ; 2        ; 0            ; 20           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[5]  ; F1    ; 2        ; 0            ; 20           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex0[6]  ; E2    ; 2        ; 0            ; 20           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[0]  ; E1    ; 2        ; 0            ; 20           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[1]  ; H6    ; 2        ; 0            ; 21           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[2]  ; H5    ; 2        ; 0            ; 21           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[3]  ; H4    ; 2        ; 0            ; 21           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[4]  ; G3    ; 2        ; 0            ; 21           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[5]  ; D2    ; 2        ; 0            ; 22           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex1[6]  ; D1    ; 2        ; 0            ; 22           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[0]  ; G5    ; 2        ; 0            ; 22           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[1]  ; G6    ; 2        ; 0            ; 23           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[2]  ; C2    ; 2        ; 0            ; 23           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[3]  ; C1    ; 2        ; 0            ; 23           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[4]  ; E3    ; 2        ; 0            ; 24           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[5]  ; E4    ; 2        ; 0            ; 24           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex2[6]  ; D3    ; 2        ; 0            ; 25           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[0]  ; F4    ; 2        ; 0            ; 23           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[1]  ; D5    ; 2        ; 0            ; 24           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[2]  ; D6    ; 2        ; 0            ; 24           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[3]  ; J4    ; 2        ; 0            ; 18           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[4]  ; L8    ; 2        ; 0            ; 19           ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[5]  ; F3    ; 2        ; 0            ; 22           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; hex3[6]  ; D4    ; 2        ; 0            ; 25           ; 3           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[0]   ; U22   ; 6        ; 50           ; 7            ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[1]   ; U21   ; 6        ; 50           ; 7            ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[2]   ; V22   ; 6        ; 50           ; 7            ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[3]   ; V21   ; 6        ; 50           ; 6            ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[4]   ; W22   ; 6        ; 50           ; 5            ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[5]   ; W21   ; 6        ; 50           ; 4            ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[6]   ; Y22   ; 6        ; 50           ; 6            ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; led[7]   ; Y21   ; 6        ; 50           ; 6            ; 2           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; red[0]   ; D9    ; 3        ; 13           ; 27           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; red[1]   ; C9    ; 3        ; 9            ; 27           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; red[2]   ; A7    ; 3        ; 11           ; 27           ; 1           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; red[3]   ; B7    ; 3        ; 11           ; 27           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
; v_sync   ; B11   ; 3        ; 22           ; 27           ; 0           ; no              ; no                     ; no            ; no              ; no         ; no            ; no       ; Off          ; 3.3-V LVTTL  ; 24mA             ; Off         ; User                 ; 0 pF ; -                    ; -                   ;
+----------+-------+----------+--------------+--------------+-------------+-----------------+------------------------+---------------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-------------+----------------------+------+----------------------+---------------------+


+------------------------------------------------------------+
; I/O Bank Usage                                             ;
+----------+------------------+---------------+--------------+
; I/O Bank ; Usage            ; VCCIO Voltage ; VREF Voltage ;
+----------+------------------+---------------+--------------+
; 1        ; 0 / 41 ( 0 % )   ; 3.3V          ; --           ;
; 2        ; 31 / 33 ( 94 % ) ; 3.3V          ; --           ;
; 3        ; 14 / 43 ( 33 % ) ; 3.3V          ; --           ;
; 4        ; 0 / 40 ( 0 % )   ; 3.3V          ; --           ;
; 5        ; 0 / 39 ( 0 % )   ; 3.3V          ; --           ;
; 6        ; 13 / 36 ( 36 % ) ; 3.3V          ; --           ;
; 7        ; 0 / 40 ( 0 % )   ; 3.3V          ; --           ;
; 8        ; 0 / 43 ( 0 % )   ; 3.3V          ; --           ;
+----------+------------------+---------------+--------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; All Package Pins                                                                                                                                                       ;
+----------+------------+----------+------------------------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
; Location ; Pad Number ; I/O Bank ; Pin Name/Usage                           ; Dir.   ; I/O Standard ; Voltage ; I/O Type   ; User Assignment ; Bus Hold ; Weak Pull Up ;
+----------+------------+----------+------------------------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
; A1       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; A2       ;            ; 3        ; VCCIO3                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; A3       ; 325        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A4       ; 324        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A5       ; 322        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A6       ; 320        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A7       ; 306        ; 3        ; red[2]                                   ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; A8       ; 304        ; 3        ; green[3]                                 ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; A9       ; 298        ; 3        ; blue[0]                                  ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; A10      ; 293        ; 3        ; blue[2]                                  ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; A11      ; 287        ; 3        ; h_sync                                   ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; A12      ; 283        ; 4        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; A13      ; 281        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A14      ; 279        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A15      ; 273        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A16      ; 271        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A17      ; 265        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A18      ; 251        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A19      ; 249        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A20      ; 247        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; A21      ;            ; 4        ; VCCIO4                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; A22      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA1      ;            ; 1        ; VCCIO1                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; AA2      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA3      ; 82         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA4      ; 85         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA5      ; 89         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA6      ; 97         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA7      ; 103        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA8      ; 111        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA9      ; 114        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA10     ; 120        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA11     ; 122        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA12     ; 128        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA13     ; 130        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA14     ; 136        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA15     ; 138        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA16     ; 140        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA17     ; 144        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA18     ; 153        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA19     ; 162        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA20     ; 164        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AA21     ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA22     ;            ; 6        ; VCCIO6                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; AB1      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AB2      ;            ; 8        ; VCCIO8                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; AB3      ; 83         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB4      ; 84         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB5      ; 88         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB6      ; 96         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB7      ; 102        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB8      ; 110        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB9      ; 113        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB10     ; 119        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB11     ; 121        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB12     ; 127        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB13     ; 129        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB14     ; 135        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB15     ; 137        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB16     ; 139        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB17     ; 143        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB18     ; 152        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB19     ; 161        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB20     ; 163        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; AB21     ;            ; 7        ; VCCIO7                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; AB22     ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B1       ;            ; 2        ; VCCIO2                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; B2       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B3       ; 326        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B4       ; 323        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B5       ; 321        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B6       ; 319        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B7       ; 305        ; 3        ; red[3]                                   ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; B8       ; 303        ; 3        ; green[0]                                 ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; B9       ; 297        ; 3        ; green[2]                                 ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; B10      ; 292        ; 3        ; blue[3]                                  ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; B11      ; 286        ; 3        ; v_sync                                   ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; B12      ; 282        ; 4        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; B13      ; 280        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B14      ; 278        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B15      ; 272        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B16      ; 270        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B17      ; 264        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B18      ; 250        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B19      ; 248        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B20      ; 246        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; B21      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B22      ;            ; 5        ; VCCIO5                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; C1       ; 8          ; 2        ; hex2[3]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; C2       ; 9          ; 2        ; hex2[2]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; C3       ; 1          ; 2        ; ~nCSO~ / RESERVED_INPUT_WITH_WEAK_PULLUP ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; N               ; no       ; On           ;
; C4       ; 0          ; 2        ; ~ASDO~ / RESERVED_INPUT_WITH_WEAK_PULLUP ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; N               ; no       ; On           ;
; C5       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; C6       ;            ; 3        ; VCCIO3                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; C7       ; 315        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; C8       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; C9       ; 310        ; 3        ; red[1]                                   ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; C10      ; 296        ; 3        ; green[1]                                 ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; C11      ;            ; 3        ; VCCIO3                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; C12      ;            ; 4        ; VCCIO4                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; C13      ; 275        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; C14      ; 260        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; C15      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; C16      ; 254        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; C17      ; 245        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; C18      ; 244        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; C19      ; 238        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; C20      ; 239        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; C21      ; 236        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; C22      ; 237        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; D1       ; 14         ; 2        ; hex1[6]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D2       ; 15         ; 2        ; hex1[5]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D3       ; 2          ; 2        ; hex2[6]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D4       ; 3          ; 2        ; hex3[6]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D5       ; 4          ; 2        ; hex3[1]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D6       ; 5          ; 2        ; hex3[2]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D7       ; 311        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; D8       ; 309        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; D9       ; 302        ; 3        ; red[0]                                   ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; D10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; D11      ; 289        ; 3        ; blue[1]                                  ; output ; 3.3-V LVTTL  ;         ; Column I/O ; Y               ; no       ; Off          ;
; D12      ; 284        ; 3        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; D13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; D14      ; 267        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; D15      ; 259        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; D16      ; 255        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; D17      ;            ; 4        ; VCCIO4                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; D18      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; D19      ; 240        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; D20      ; 241        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; D21      ; 229        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; D22      ; 230        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; E1       ; 20         ; 2        ; hex1[0]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; E2       ; 21         ; 2        ; hex0[6]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; E3       ; 6          ; 2        ; hex2[4]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; E4       ; 7          ; 2        ; hex2[5]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; E5       ;            ;          ; VCCD_PLL3                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; E6       ;            ;          ; VCCA_PLL3                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; E7       ; 316        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; E8       ; 308        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; E9       ; 301        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; E10      ;            ; 3        ; VCCIO3                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; E11      ; 288        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; E12      ; 285        ; 3        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; E13      ;            ; 4        ; VCCIO4                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; E14      ; 266        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; E15      ; 256        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; E16      ;            ;          ; GNDA_PLL2                                ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; E17      ;            ;          ; GND_PLL2                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; E18      ; 243        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; E19      ; 242        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; E20      ; 234        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; E21      ; 227        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; E22      ; 228        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; F1       ; 22         ; 2        ; hex0[5]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; F2       ; 23         ; 2        ; hex0[4]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; F3       ; 13         ; 2        ; hex3[5]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; F4       ; 10         ; 2        ; hex3[0]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; F5       ;            ;          ; GND_PLL3                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F6       ;            ;          ; GND_PLL3                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F7       ;            ;          ; GNDA_PLL3                                ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F8       ; 312        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F9       ; 307        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F10      ; 295        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F11      ; 294        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F12      ; 276        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F13      ; 269        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F14      ; 268        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F15      ; 262        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; F16      ;            ;          ; VCCA_PLL2                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; F17      ;            ;          ; VCCD_PLL2                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; F18      ;            ;          ; GND_PLL2                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F19      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F20      ; 235        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; F21      ; 223        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; F22      ; 224        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; G1       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; G2       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; G3       ; 16         ; 2        ; hex1[4]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; G4       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; G5       ; 12         ; 2        ; hex2[0]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; G6       ; 11         ; 2        ; hex2[1]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; G7       ; 317        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; G8       ; 313        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; G9       ;            ; 3        ; VCCIO3                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; G10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; G11      ; 291        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; G12      ; 277        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; G13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; G14      ;            ; 4        ; VCCIO4                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; G15      ; 261        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; G16      ; 252        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; G17      ; 231        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; G18      ; 232        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; G19      ;            ; 5        ; VCCIO5                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; G20      ; 233        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; G21      ; 221        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; G22      ; 222        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; H1       ; 24         ; 2        ; hex0[3]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; H2       ; 25         ; 2        ; hex0[2]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; H3       ; 27         ; 2        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; H4       ; 17         ; 2        ; hex1[3]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; H5       ; 18         ; 2        ; hex1[2]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; H6       ; 19         ; 2        ; hex1[1]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; H7       ; 318        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H8       ; 314        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H9       ; 300        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H10      ; 299        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H11      ; 290        ; 3        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H12      ; 274        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H13      ; 263        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H14      ; 257        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H15      ; 253        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; H16      ; 219        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; H17      ; 226        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; H18      ; 225        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; H19      ; 214        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; H20      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; H21      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; H22      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; J1       ; 29         ; 2        ; hex0[1]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; J2       ; 30         ; 2        ; hex0[0]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; J3       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; J4       ; 28         ; 2        ; hex3[3]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; J5       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; J6       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; J7       ;            ; 2        ; VCCIO2                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; J8       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; J9       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; J10      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; J11      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; J12      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; J13      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; J14      ; 258        ; 4        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; J15      ; 220        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; J16      ;            ; 5        ; VCCIO5                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; J17      ; 218        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; J18      ; 217        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; J19      ; 216        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; J20      ; 213        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; J21      ; 211        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; J22      ; 212        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; K1       ; 37         ; 2        ; ^nCE                                     ;        ;              ;         ; --         ;                 ; --       ; --           ;
; K2       ; 32         ; 2        ; #TCK                                     ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; K3       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K4       ; 36         ; 2        ; ^DATA0                                   ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; K5       ; 31         ; 2        ; #TDI                                     ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; K6       ; 33         ; 2        ; #TMS                                     ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; K7       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K8       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; K9       ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K11      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K12      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K14      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K15      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; K16      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K17      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; K18      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; K19      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K20      ; 215        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; K21      ; 209        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; K22      ; 210        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; L1       ; 38         ; 2        ; clk_50MHz                                ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; L2       ; 39         ; 2        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; L3       ;            ; 2        ; VCCIO2                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; L4       ; 40         ; 2        ; ^nCONFIG                                 ;        ;              ;         ; --         ;                 ; --       ; --           ;
; L5       ; 34         ; 2        ; #TDO                                     ; output ;              ;         ; --         ;                 ; --       ; --           ;
; L6       ; 35         ; 2        ; ^DCLK                                    ;        ;              ;         ; --         ;                 ; --       ; --           ;
; L7       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; L8       ; 26         ; 2        ; hex3[4]                                  ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; L9       ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L11      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L12      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L14      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L15      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; L16      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; L17      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; L18      ; 208        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; L19      ; 207        ; 5        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; L20      ;            ; 5        ; VCCIO5                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; L21      ; 205        ; 5        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; L22      ; 206        ; 5        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; M1       ; 41         ; 1        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; M2       ; 42         ; 1        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; M3       ;            ; 1        ; VCCIO1                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; M4       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M5       ; 43         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; M6       ; 44         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; M7       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M8       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M9       ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M11      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M12      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M14      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M15      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M16      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M17      ; 198        ; 6        ; ^MSEL0                                   ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M18      ; 202        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; M19      ; 201        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; M20      ;            ; 6        ; VCCIO6                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; M21      ; 203        ; 6        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; M22      ; 204        ; 6        ; GND+                                     ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; N1       ; 45         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N2       ; 46         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N3       ; 51         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N4       ; 52         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N5       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; N6       ; 49         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N7       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N8       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; N9       ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N11      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N12      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N14      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N15      ; 194        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N16      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N17      ; 197        ; 6        ; ^MSEL1                                   ;        ;              ;         ; --         ;                 ; --       ; --           ;
; N18      ; 196        ; 6        ; ^CONF_DONE                               ;        ;              ;         ; --         ;                 ; --       ; --           ;
; N19      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N20      ; 195        ; 6        ; ^nSTATUS                                 ;        ;              ;         ; --         ;                 ; --       ; --           ;
; N21      ; 199        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; N22      ; 200        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P1       ; 47         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P2       ; 48         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P3       ; 50         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P4       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P5       ; 55         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P6       ; 56         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P7       ;            ; 1        ; VCCIO1                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; P8       ; 95         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; P9       ; 94         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; P10      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P11      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P12      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P13      ;            ;          ; VCCINT                                   ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P14      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P15      ; 193        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P16      ;            ; 6        ; VCCIO6                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; P17      ; 186        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P18      ; 187        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; P19      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P20      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P21      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P22      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; R1       ; 57         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R2       ; 58         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R3       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R4       ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; R5       ; 63         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R6       ; 64         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R7       ; 54         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R8       ; 53         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R9       ; 109        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R10      ; 108        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R11      ; 116        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R12      ; 134        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R13      ; 145        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R14      ; 150        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R15      ; 151        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R16      ; 155        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; R17      ; 177        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R18      ; 184        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R19      ; 185        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R20      ; 192        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; R21      ; 190        ; 6        ; button3                                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; R22      ; 191        ; 6        ; button4                                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; T1       ; 59         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; T2       ; 60         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; T3       ; 69         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; T4       ;            ; 1        ; VCCIO1                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; T5       ; 67         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; T6       ; 68         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; T7       ; 91         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; T8       ; 90         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; T9       ;            ; 8        ; VCCIO8                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; T10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T11      ; 115        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; T12      ; 131        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; T13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T14      ;            ; 7        ; VCCIO7                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; T15      ; 147        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; T16      ; 156        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; T17      ;            ;          ; GND_PLL4                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T18      ; 171        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; T19      ;            ; 6        ; VCCIO6                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; T20      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T21      ; 188        ; 6        ; button1                                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; T22      ; 189        ; 6        ; button2                                  ; input  ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; U1       ; 61         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U2       ; 62         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U3       ; 70         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U4       ; 80         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U5       ;            ;          ; GND_PLL1                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U6       ;            ;          ; VCCD_PLL1                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U7       ;            ;          ; VCCA_PLL1                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U8       ; 92         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; U9       ; 106        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; U10      ; 107        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; U11      ; 123        ; 8        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; U12      ; 124        ; 8        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; U13      ; 132        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; U14      ; 146        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; U15      ; 157        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; U16      ;            ;          ; VCCA_PLL4                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U17      ;            ;          ; VCCD_PLL4                                ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U18      ; 170        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U19      ; 172        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U20      ; 176        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; U21      ; 182        ; 6        ; led[1]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; U22      ; 183        ; 6        ; led[0]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; V1       ; 65         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; V2       ; 66         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; V3       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V4       ; 81         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; V5       ;            ;          ; GND_PLL1                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V6       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V7       ;            ;          ; GNDA_PLL1                                ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V8       ; 98         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; V9       ; 101        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; V10      ;            ; 8        ; VCCIO8                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; V11      ; 118        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; V12      ; 126        ; 7        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; V13      ;            ; 7        ; VCCIO7                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; V14      ; 142        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; V15      ; 158        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; V16      ;            ;          ; GNDA_PLL4                                ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V17      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V18      ;            ;          ; GND_PLL4                                 ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V19      ; 166        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; V20      ; 173        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; V21      ; 180        ; 6        ; led[3]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; V22      ; 181        ; 6        ; led[2]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; W1       ; 71         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; W2       ; 72         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; W3       ; 75         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; W4       ; 76         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; W5       ; 79         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; W6       ;            ; 8        ; VCCIO8                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; W7       ; 99         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W8       ; 100        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W9       ; 105        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W10      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W11      ; 117        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W12      ; 125        ; 7        ; GND+                                     ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; W13      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W14      ; 141        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W15      ; 149        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W16      ; 160        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; W17      ;            ; 7        ; VCCIO7                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; W18      ;            ;          ; NC                                       ;        ;              ;         ; --         ;                 ; --       ; --           ;
; W19      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W20      ; 167        ; 6        ; ~LVDS91p/nCEO~                           ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; N               ; no       ; Off          ;
; W21      ; 174        ; 6        ; led[5]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; W22      ; 175        ; 6        ; led[4]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; Y1       ; 73         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y2       ; 74         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y3       ; 77         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y4       ; 78         ; 1        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y5       ; 86         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y6       ; 87         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y7       ; 93         ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y8       ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; Y9       ; 104        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y10      ; 112        ; 8        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y11      ;            ; 8        ; VCCIO8                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; Y12      ;            ; 7        ; VCCIO7                                   ; power  ;              ; 3.3V    ; --         ;                 ; --       ; --           ;
; Y13      ; 133        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y14      ; 148        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y15      ;            ;          ; GND                                      ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; Y16      ; 154        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y17      ; 159        ; 7        ; GND*                                     ;        ;              ;         ; Column I/O ;                 ; no       ; Off          ;
; Y18      ; 165        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y19      ; 168        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y20      ; 169        ; 6        ; GND*                                     ;        ;              ;         ; Row I/O    ;                 ; no       ; Off          ;
; Y21      ; 178        ; 6        ; led[7]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
; Y22      ; 179        ; 6        ; led[6]                                   ; output ; 3.3-V LVTTL  ;         ; Row I/O    ; Y               ; no       ; Off          ;
+----------+------------+----------+------------------------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
Note: Pin directions (input, output or bidir) are based on device operating in user mode.


+-------------------------------------------------------------------------------+
; Output Pin Default Load For Reported TCO                                      ;
+----------------------------------+-------+------------------------------------+
; I/O Standard                     ; Load  ; Termination Resistance             ;
+----------------------------------+-------+------------------------------------+
; 3.3-V LVTTL                      ; 0 pF  ; Not Available                      ;
; 3.3-V LVCMOS                     ; 0 pF  ; Not Available                      ;
; 2.5 V                            ; 0 pF  ; Not Available                      ;
; 1.8 V                            ; 0 pF  ; Not Available                      ;
; 1.5 V                            ; 0 pF  ; Not Available                      ;
; 3.3-V PCI                        ; 10 pF ; 25 Ohm (Parallel)                  ;
; 3.3-V PCI-X                      ; 10 pF ; 25 Ohm (Parallel)                  ;
; SSTL-2 Class I                   ; 0 pF  ; 50 Ohm (Parallel), 25 Ohm (Serial) ;
; SSTL-2 Class II                  ; 0 pF  ; 25 Ohm (Parallel), 25 Ohm (Serial) ;
; SSTL-18 Class I                  ; 0 pF  ; 50 Ohm (Parallel), 25 Ohm (Serial) ;
; SSTL-18 Class II                 ; 0 pF  ; 25 Ohm (Parallel), 25 Ohm (Serial) ;
; 1.5-V HSTL Class I               ; 0 pF  ; 50 Ohm (Parallel)                  ;
; 1.5-V HSTL Class II              ; 0 pF  ; 25 Ohm (Parallel)                  ;
; 1.8-V HSTL Class I               ; 0 pF  ; 50 Ohm (Parallel)                  ;
; 1.8-V HSTL Class II              ; 0 pF  ; 25 Ohm (Parallel)                  ;
; Differential SSTL-2              ; 0 pF  ; (See SSTL-2)                       ;
; Differential 2.5-V SSTL Class II ; 0 pF  ; (See SSTL-2 Class II)              ;
; Differential 1.8-V SSTL Class I  ; 0 pF  ; (See 1.8-V SSTL Class I)           ;
; Differential 1.8-V SSTL Class II ; 0 pF  ; (See 1.8-V SSTL Class II)          ;
; Differential 1.5-V HSTL Class I  ; 0 pF  ; (See 1.5-V HSTL Class I)           ;
; Differential 1.5-V HSTL Class II ; 0 pF  ; (See 1.5-V HSTL Class II)          ;
; Differential 1.8-V HSTL Class I  ; 0 pF  ; (See 1.8-V HSTL Class I)           ;
; Differential 1.8-V HSTL Class II ; 0 pF  ; (See 1.8-V HSTL Class II)          ;
; LVDS                             ; 0 pF  ; 100 Ohm (Differential)             ;
; mini-LVDS                        ; 0 pF  ; 100 Ohm (Differential)             ;
; RSDS                             ; 0 pF  ; 100 Ohm (Differential)             ;
; Simple RSDS                      ; 0 pF  ; Not Available                      ;
; Differential LVPECL              ; 0 pF  ; 100 Ohm (Differential)             ;
+----------------------------------+-------+------------------------------------+
Note: User assignments will override these defaults. The user specified values are listed in the Output Pins and Bidir Pins tables.


+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Utilization by Entity                                                                                                                                                                                                                                                                                                                                             ;
+------------------------------------------+-------------+---------------------------+---------------+-------------+------+--------------+---------+-----------+------+--------------+--------------+-------------------+------------------+-------------------------------------------------------------------------------------------------------------------------+--------------+
; Compilation Hierarchy Node               ; Logic Cells ; Dedicated Logic Registers ; I/O Registers ; Memory Bits ; M4Ks ; DSP Elements ; DSP 9x9 ; DSP 18x18 ; Pins ; Virtual Pins ; LUT-Only LCs ; Register-Only LCs ; LUT/Register LCs ; Full Hierarchy Name                                                                                                     ; Library Name ;
+------------------------------------------+-------------+---------------------------+---------------+-------------+------+--------------+---------+-----------+------+--------------+--------------+-------------------+------------------+-------------------------------------------------------------------------------------------------------------------------+--------------+
; |TotalScheme                             ; 7148 (0)    ; 1086 (0)                  ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 55   ; 0            ; 6062 (0)     ; 52 (0)            ; 1034 (0)         ; |TotalScheme                                                                                                            ; work         ;
;    |Arkanoid:inst|                       ; 7110 (3971) ; 1049 (1049)               ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6059 (2920)  ; 31 (31)           ; 1020 (1020)      ; |TotalScheme|Arkanoid:inst                                                                                              ;              ;
;       |lpm_divide:Div0|                  ; 515 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 515 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div0                                                                              ;              ;
;          |lpm_divide_7so:auto_generated| ; 515 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 515 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated                                                ;              ;
;             |abs_divider_kbg:divider|    ; 515 (35)    ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 515 (35)     ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider                        ;              ;
;                |alt_u_div_k2f:divider|   ; 449 (449)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 449 (449)    ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider  ;              ;
;                |lpm_abs_0s9:my_abs_num|  ; 31 (31)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 31 (31)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num ;              ;
;       |lpm_divide:Div1|                  ; 515 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 515 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div1                                                                              ;              ;
;          |lpm_divide_7so:auto_generated| ; 515 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 515 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div1|lpm_divide_7so:auto_generated                                                ;              ;
;             |abs_divider_kbg:divider|    ; 515 (35)    ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 515 (35)     ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div1|lpm_divide_7so:auto_generated|abs_divider_kbg:divider                        ;              ;
;                |alt_u_div_k2f:divider|   ; 449 (449)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 449 (449)    ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div1|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider  ;              ;
;                |lpm_abs_0s9:my_abs_num|  ; 31 (31)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 31 (31)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div1|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num ;              ;
;       |lpm_divide:Div2|                  ; 553 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 553 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div2                                                                              ;              ;
;          |lpm_divide_8so:auto_generated| ; 553 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 553 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated                                                ;              ;
;             |abs_divider_lbg:divider|    ; 553 (10)    ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 553 (10)     ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider                        ;              ;
;                |alt_u_div_m2f:divider|   ; 511 (511)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 511 (511)    ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|alt_u_div_m2f:divider  ;              ;
;                |lpm_abs_0s9:my_abs_num|  ; 32 (32)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 32 (32)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|lpm_abs_0s9:my_abs_num ;              ;
;       |lpm_divide:Div3|                  ; 553 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 553 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div3                                                                              ;              ;
;          |lpm_divide_8so:auto_generated| ; 553 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 553 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div3|lpm_divide_8so:auto_generated                                                ;              ;
;             |abs_divider_lbg:divider|    ; 553 (10)    ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 553 (10)     ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div3|lpm_divide_8so:auto_generated|abs_divider_lbg:divider                        ;              ;
;                |alt_u_div_m2f:divider|   ; 511 (511)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 511 (511)    ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div3|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|alt_u_div_m2f:divider  ;              ;
;                |lpm_abs_0s9:my_abs_num|  ; 32 (32)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 32 (32)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Div3|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|lpm_abs_0s9:my_abs_num ;              ;
;       |lpm_divide:Mod0|                  ; 502 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 502 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod0                                                                              ;              ;
;          |lpm_divide_ako:auto_generated| ; 502 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 502 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod0|lpm_divide_ako:auto_generated                                                ;              ;
;             |abs_divider_kbg:divider|    ; 502 (10)    ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 502 (10)     ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod0|lpm_divide_ako:auto_generated|abs_divider_kbg:divider                        ;              ;
;                |alt_u_div_k2f:divider|   ; 459 (459)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 459 (459)    ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod0|lpm_divide_ako:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider  ;              ;
;                |lpm_abs_0s9:my_abs_num|  ; 33 (33)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 33 (33)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod0|lpm_divide_ako:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num ;              ;
;       |lpm_divide:Mod1|                  ; 501 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 501 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod1                                                                              ;              ;
;          |lpm_divide_ako:auto_generated| ; 501 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 501 (0)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod1|lpm_divide_ako:auto_generated                                                ;              ;
;             |abs_divider_kbg:divider|    ; 501 (9)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 501 (9)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod1|lpm_divide_ako:auto_generated|abs_divider_kbg:divider                        ;              ;
;                |alt_u_div_k2f:divider|   ; 459 (459)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 459 (459)    ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod1|lpm_divide_ako:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider  ;              ;
;                |lpm_abs_0s9:my_abs_num|  ; 33 (33)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 33 (33)      ; 0 (0)             ; 0 (0)            ; |TotalScheme|Arkanoid:inst|lpm_divide:Mod1|lpm_divide_ako:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num ;              ;
;    |ClockDivider:inst1|                  ; 1 (1)       ; 1 (1)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 1 (1)            ; |TotalScheme|ClockDivider:inst1                                                                                         ;              ;
;    |Debouncer:inst2|                     ; 9 (9)       ; 9 (9)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 5 (5)             ; 4 (4)            ; |TotalScheme|Debouncer:inst2                                                                                            ;              ;
;    |Debouncer:inst3|                     ; 10 (10)     ; 9 (9)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 1 (1)        ; 6 (6)             ; 3 (3)            ; |TotalScheme|Debouncer:inst3                                                                                            ;              ;
;    |Debouncer:inst4|                     ; 10 (10)     ; 9 (9)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 1 (1)        ; 5 (5)             ; 4 (4)            ; |TotalScheme|Debouncer:inst4                                                                                            ;              ;
;    |Debouncer:inst5|                     ; 10 (10)     ; 9 (9)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 1 (1)        ; 5 (5)             ; 4 (4)            ; |TotalScheme|Debouncer:inst5                                                                                            ;              ;
+------------------------------------------+-------------+---------------------------+---------------+-------------+------+--------------+---------+-----------+------+--------------+--------------+-------------------+------------------+-------------------------------------------------------------------------------------------------------------------------+--------------+
Note: For table entries with two numbers listed, the numbers in parentheses indicate the number of resources of the given type used by the specific entity alone. The numbers listed outside of parentheses indicate the total resources of the given type used by the specific entity and all of its sub-entities in the hierarchy.


+------------------------------------------------------------------------------------+
; Delay Chain Summary                                                                ;
+-----------+----------+---------------+---------------+-----------------------+-----+
; Name      ; Pin Type ; Pad to Core 0 ; Pad to Core 1 ; Pad to Input Register ; TCO ;
+-----------+----------+---------------+---------------+-----------------------+-----+
; h_sync    ; Output   ; --            ; --            ; --                    ; --  ;
; v_sync    ; Output   ; --            ; --            ; --                    ; --  ;
; blue[3]   ; Output   ; --            ; --            ; --                    ; --  ;
; blue[2]   ; Output   ; --            ; --            ; --                    ; --  ;
; blue[1]   ; Output   ; --            ; --            ; --                    ; --  ;
; blue[0]   ; Output   ; --            ; --            ; --                    ; --  ;
; green[3]  ; Output   ; --            ; --            ; --                    ; --  ;
; green[2]  ; Output   ; --            ; --            ; --                    ; --  ;
; green[1]  ; Output   ; --            ; --            ; --                    ; --  ;
; green[0]  ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[6]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[5]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[4]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[3]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[2]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[1]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex0[0]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[6]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[5]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[4]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[3]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[2]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[1]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex1[0]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[6]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[5]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[4]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[3]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[2]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[1]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex2[0]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[6]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[5]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[4]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[3]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[2]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[1]   ; Output   ; --            ; --            ; --                    ; --  ;
; hex3[0]   ; Output   ; --            ; --            ; --                    ; --  ;
; led[7]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[6]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[5]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[4]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[3]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[2]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[1]    ; Output   ; --            ; --            ; --                    ; --  ;
; led[0]    ; Output   ; --            ; --            ; --                    ; --  ;
; red[3]    ; Output   ; --            ; --            ; --                    ; --  ;
; red[2]    ; Output   ; --            ; --            ; --                    ; --  ;
; red[1]    ; Output   ; --            ; --            ; --                    ; --  ;
; red[0]    ; Output   ; --            ; --            ; --                    ; --  ;
; clk_50MHz ; Input    ; (0) 325 ps    ; (0) 325 ps    ; --                    ; --  ;
; button1   ; Input    ; (6) 4358 ps   ; (6) 4358 ps   ; --                    ; --  ;
; button2   ; Input    ; (6) 4358 ps   ; (6) 4358 ps   ; --                    ; --  ;
; button3   ; Input    ; (6) 4358 ps   ; (6) 4358 ps   ; --                    ; --  ;
; button4   ; Input    ; (6) 4358 ps   ; (6) 4358 ps   ; --                    ; --  ;
+-----------+----------+---------------+---------------+-----------------------+-----+


+--------------------------------------------------------------------+
; Pad To Core Delay Chain Fanout                                     ;
+--------------------------------------+-------------------+---------+
; Source Pin / Fanout                  ; Pad To Core Index ; Setting ;
+--------------------------------------+-------------------+---------+
; clk_50MHz                            ;                   ;         ;
; button1                              ;                   ;         ;
;      - Debouncer:inst2|button_reg[0] ; 0                 ; 6       ;
; button2                              ;                   ;         ;
;      - Debouncer:inst3|button_reg[0] ; 0                 ; 6       ;
; button3                              ;                   ;         ;
;      - Debouncer:inst4|button_reg[0] ; 0                 ; 6       ;
; button4                              ;                   ;         ;
;      - Debouncer:inst5|button_reg[0] ; 1                 ; 6       ;
+--------------------------------------+-------------------+---------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Control Signals                                                                                                                                                        ;
+------------------------------+--------------------+---------+---------------------------+--------+----------------------+------------------+---------------------------+
; Name                         ; Location           ; Fan-Out ; Usage                     ; Global ; Global Resource Used ; Global Line Name ; Enable Signal Source Name ;
+------------------------------+--------------------+---------+---------------------------+--------+----------------------+------------------+---------------------------+
; Arkanoid:inst|Equal1~10      ; LCCOMB_X21_Y13_N0  ; 32      ; Sync. clear               ; no     ; --                   ; --               ; --                        ;
; Arkanoid:inst|LessThan132~10 ; LCCOMB_X32_Y19_N22 ; 36      ; Sync. clear               ; no     ; --                   ; --               ; --                        ;
; Arkanoid:inst|always2~10     ; LCCOMB_X32_Y11_N6  ; 3       ; Clock enable              ; no     ; --                   ; --               ; --                        ;
; Arkanoid:inst|always2~11     ; LCCOMB_X32_Y10_N30 ; 3       ; Clock enable              ; no     ; --                   ; --               ; --                        ;
; Arkanoid:inst|always2~12     ; LCCOMB_X31_Y13_N18 ; 3       ; Clock enable              ; no     ; --                   ; --               ; --                        ;
; Arkanoid:inst|always2~9      ; LCCOMB_X33_Y13_N30 ; 3       ; Clock enable              ; no     ; --                   ; --               ; --                        ;
; Arkanoid:inst|game_state~4   ; LCCOMB_X31_Y13_N4  ; 37      ; Clock enable, Sync. clear ; no     ; --                   ; --               ; --                        ;
; ClockDivider:inst1|clk25MHz_ ; LCFF_X1_Y13_N29    ; 1085    ; Clock                     ; yes    ; Global Clock         ; GCLK0            ; --                        ;
; clk_50MHz                    ; PIN_L1             ; 1       ; Clock                     ; no     ; --                   ; --               ; --                        ;
+------------------------------+--------------------+---------+---------------------------+--------+----------------------+------------------+---------------------------+


+--------------------------------------------------------------------------------------------------------------------------------+
; Global & Other Fast Signals                                                                                                    ;
+------------------------------+-----------------+---------+----------------------+------------------+---------------------------+
; Name                         ; Location        ; Fan-Out ; Global Resource Used ; Global Line Name ; Enable Signal Source Name ;
+------------------------------+-----------------+---------+----------------------+------------------+---------------------------+
; ClockDivider:inst1|clk25MHz_ ; LCFF_X1_Y13_N29 ; 1085    ; Global Clock         ; GCLK0            ; --                        ;
+------------------------------+-----------------+---------+----------------------+------------------+---------------------------+


+-------------------------------------------------------------------------------------------------------------+
; Non-Global High Fan-Out Signals                                                                             ;
+---------------------------------------------------------------------------------------------------+---------+
; Name                                                                                              ; Fan-Out ;
+---------------------------------------------------------------------------------------------------+---------+
; Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|quotient[3]~3 ; 197     ;
; Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|quotient[2]~2 ; 197     ;
; Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|quotient[0]~1 ; 197     ;
; Arkanoid:inst|lpm_divide:Div2|lpm_divide_8so:auto_generated|abs_divider_lbg:divider|quotient[1]~0 ; 197     ;
; Arkanoid:inst|ball_direction~17                                                                   ; 142     ;
; Arkanoid:inst|Decoder3~1                                                                          ; 131     ;
; Arkanoid:inst|Decoder2~12                                                                         ; 129     ;
; Arkanoid:inst|Decoder3~33                                                                         ; 124     ;
; Arkanoid:inst|Decoder2~13                                                                         ; 122     ;
; Arkanoid:inst|game_state                                                                          ; 110     ;
; Arkanoid:inst|Decoder2~8                                                                          ; 100     ;
; Arkanoid:inst|field~885                                                                           ; 96      ;
; Arkanoid:inst|field~1017                                                                          ; 94      ;
; Arkanoid:inst|Add14~65                                                                            ; 93      ;
; Arkanoid:inst|field~819                                                                           ; 92      ;
; Arkanoid:inst|Add9~65                                                                             ; 89      ;
; Arkanoid:inst|Selector37~3                                                                        ; 83      ;
; Arkanoid:inst|platform1_position~61                                                               ; 79      ;
; Arkanoid:inst|platform2_position~4                                                                ; 73      ;
; Arkanoid:inst|Decoder2~11                                                                         ; 72      ;
; Arkanoid:inst|platform1_position~60                                                               ; 69      ;
; Arkanoid:inst|field~1451                                                                          ; 65      ;
; Arkanoid:inst|field~951                                                                           ; 64      ;
; Arkanoid:inst|platform1_position~75                                                               ; 56      ;
; Arkanoid:inst|ball_y~25                                                                           ; 55      ;
; Arkanoid:inst|LessThan137~0                                                                       ; 43      ;
; Arkanoid:inst|ball_x~28                                                                           ; 43      ;
; Debouncer:inst3|debounced                                                                         ; 42      ;
; Arkanoid:inst|Decoder2~14                                                                         ; 41      ;
; Arkanoid:inst|player2_score~2                                                                     ; 37      ;
; Arkanoid:inst|game_state~4                                                                        ; 37      ;
; Arkanoid:inst|player1_score~1                                                                     ; 36      ;
; Arkanoid:inst|LessThan132~10                                                                      ; 36      ;
; Arkanoid:inst|Decoder2~9                                                                          ; 36      ;
; Arkanoid:inst|button2_state                                                                       ; 36      ;
; Arkanoid:inst|Add15~60                                                                            ; 36      ;
; Arkanoid:inst|Add16~60                                                                            ; 36      ;
; Arkanoid:inst|ball_y~27                                                                           ; 35      ;
; Arkanoid:inst|platform2_position~84                                                               ; 35      ;
; Arkanoid:inst|field~710                                                                           ; 34      ;
; Arkanoid:inst|game_state~3                                                                        ; 34      ;
; Arkanoid:inst|platform1_position~76                                                               ; 33      ;
; Arkanoid:inst|Add13~62                                                                            ; 33      ;
; Arkanoid:inst|Add7~62                                                                             ; 33      ;
; Arkanoid:inst|field~1820                                                                          ; 32      ;
; Arkanoid:inst|field~1755                                                                          ; 32      ;
; Arkanoid:inst|field~1658                                                                          ; 32      ;
; Arkanoid:inst|field~1656                                                                          ; 32      ;
; Arkanoid:inst|field~1591                                                                          ; 32      ;
; Arkanoid:inst|field~1551                                                                          ; 32      ;
+---------------------------------------------------------------------------------------------------+---------+


+------------------------------------------------------+
; Interconnect Usage Summary                           ;
+----------------------------+-------------------------+
; Interconnect Resource Type ; Usage                   ;
+----------------------------+-------------------------+
; Block interconnects        ; 9,680 / 54,004 ( 18 % ) ;
; C16 interconnects          ; 106 / 2,100 ( 5 % )     ;
; C4 interconnects           ; 5,746 / 36,000 ( 16 % ) ;
; Direct links               ; 2,159 / 54,004 ( 4 % )  ;
; Global clocks              ; 1 / 16 ( 6 % )          ;
; Local interconnects        ; 3,489 / 18,752 ( 19 % ) ;
; R24 interconnects          ; 197 / 1,900 ( 10 % )    ;
; R4 interconnects           ; 6,847 / 46,920 ( 15 % ) ;
+----------------------------+-------------------------+


+-----------------------------------------------------------------------------+
; LAB Logic Elements                                                          ;
+---------------------------------------------+-------------------------------+
; Number of Logic Elements  (Average = 13.72) ; Number of LABs  (Total = 521) ;
+---------------------------------------------+-------------------------------+
; 1                                           ; 22                            ;
; 2                                           ; 16                            ;
; 3                                           ; 32                            ;
; 4                                           ; 7                             ;
; 5                                           ; 1                             ;
; 6                                           ; 4                             ;
; 7                                           ; 2                             ;
; 8                                           ; 1                             ;
; 9                                           ; 3                             ;
; 10                                          ; 0                             ;
; 11                                          ; 3                             ;
; 12                                          ; 1                             ;
; 13                                          ; 0                             ;
; 14                                          ; 7                             ;
; 15                                          ; 3                             ;
; 16                                          ; 419                           ;
+---------------------------------------------+-------------------------------+


+--------------------------------------------------------------------+
; LAB-wide Signals                                                   ;
+------------------------------------+-------------------------------+
; LAB-wide Signals  (Average = 0.38) ; Number of LABs  (Total = 521) ;
+------------------------------------+-------------------------------+
; 1 Clock                            ; 189                           ;
; 1 Clock enable                     ; 5                             ;
; 1 Sync. clear                      ; 4                             ;
+------------------------------------+-------------------------------+


+------------------------------------------------------------------------------+
; LAB Signals Sourced                                                          ;
+----------------------------------------------+-------------------------------+
; Number of Signals Sourced  (Average = 15.18) ; Number of LABs  (Total = 521) ;
+----------------------------------------------+-------------------------------+
; 0                                            ; 4                             ;
; 1                                            ; 24                            ;
; 2                                            ; 17                            ;
; 3                                            ; 31                            ;
; 4                                            ; 7                             ;
; 5                                            ; 1                             ;
; 6                                            ; 3                             ;
; 7                                            ; 4                             ;
; 8                                            ; 1                             ;
; 9                                            ; 0                             ;
; 10                                           ; 1                             ;
; 11                                           ; 5                             ;
; 12                                           ; 1                             ;
; 13                                           ; 1                             ;
; 14                                           ; 43                            ;
; 15                                           ; 91                            ;
; 16                                           ; 110                           ;
; 17                                           ; 19                            ;
; 18                                           ; 10                            ;
; 19                                           ; 14                            ;
; 20                                           ; 16                            ;
; 21                                           ; 10                            ;
; 22                                           ; 61                            ;
; 23                                           ; 13                            ;
; 24                                           ; 10                            ;
; 25                                           ; 3                             ;
; 26                                           ; 3                             ;
; 27                                           ; 6                             ;
; 28                                           ; 2                             ;
; 29                                           ; 4                             ;
; 30                                           ; 2                             ;
; 31                                           ; 0                             ;
; 32                                           ; 4                             ;
+----------------------------------------------+-------------------------------+


+---------------------------------------------------------------------------------+
; LAB Signals Sourced Out                                                         ;
+-------------------------------------------------+-------------------------------+
; Number of Signals Sourced Out  (Average = 8.48) ; Number of LABs  (Total = 521) ;
+-------------------------------------------------+-------------------------------+
; 0                                               ; 4                             ;
; 1                                               ; 74                            ;
; 2                                               ; 79                            ;
; 3                                               ; 12                            ;
; 4                                               ; 8                             ;
; 5                                               ; 5                             ;
; 6                                               ; 14                            ;
; 7                                               ; 4                             ;
; 8                                               ; 17                            ;
; 9                                               ; 53                            ;
; 10                                              ; 47                            ;
; 11                                              ; 52                            ;
; 12                                              ; 19                            ;
; 13                                              ; 31                            ;
; 14                                              ; 17                            ;
; 15                                              ; 5                             ;
; 16                                              ; 65                            ;
; 17                                              ; 4                             ;
; 18                                              ; 1                             ;
; 19                                              ; 0                             ;
; 20                                              ; 1                             ;
; 21                                              ; 1                             ;
; 22                                              ; 0                             ;
; 23                                              ; 1                             ;
; 24                                              ; 1                             ;
; 25                                              ; 0                             ;
; 26                                              ; 0                             ;
; 27                                              ; 2                             ;
; 28                                              ; 1                             ;
; 29                                              ; 2                             ;
; 30                                              ; 1                             ;
+-------------------------------------------------+-------------------------------+


+------------------------------------------------------------------------------+
; LAB Distinct Inputs                                                          ;
+----------------------------------------------+-------------------------------+
; Number of Distinct Inputs  (Average = 16.41) ; Number of LABs  (Total = 521) ;
+----------------------------------------------+-------------------------------+
; 0                                            ; 0                             ;
; 1                                            ; 1                             ;
; 2                                            ; 40                            ;
; 3                                            ; 20                            ;
; 4                                            ; 16                            ;
; 5                                            ; 7                             ;
; 6                                            ; 2                             ;
; 7                                            ; 8                             ;
; 8                                            ; 1                             ;
; 9                                            ; 4                             ;
; 10                                           ; 1                             ;
; 11                                           ; 23                            ;
; 12                                           ; 12                            ;
; 13                                           ; 27                            ;
; 14                                           ; 41                            ;
; 15                                           ; 21                            ;
; 16                                           ; 25                            ;
; 17                                           ; 28                            ;
; 18                                           ; 24                            ;
; 19                                           ; 14                            ;
; 20                                           ; 42                            ;
; 21                                           ; 6                             ;
; 22                                           ; 56                            ;
; 23                                           ; 13                            ;
; 24                                           ; 9                             ;
; 25                                           ; 14                            ;
; 26                                           ; 7                             ;
; 27                                           ; 11                            ;
; 28                                           ; 9                             ;
; 29                                           ; 8                             ;
; 30                                           ; 20                            ;
; 31                                           ; 3                             ;
; 32                                           ; 4                             ;
; 33                                           ; 4                             ;
+----------------------------------------------+-------------------------------+


+-------------------------------------------------------------------------+
; Fitter Device Options                                                   ;
+----------------------------------------------+--------------------------+
; Option                                       ; Setting                  ;
+----------------------------------------------+--------------------------+
; Enable user-supplied start-up clock (CLKUSR) ; Off                      ;
; Enable device-wide reset (DEV_CLRn)          ; Off                      ;
; Enable device-wide output enable (DEV_OE)    ; Off                      ;
; Enable INIT_DONE output                      ; Off                      ;
; Configuration scheme                         ; Active Serial            ;
; Error detection CRC                          ; Off                      ;
; nCEO                                         ; As output driving ground ;
; ASDO,nCSO                                    ; As input tri-stated      ;
; Reserve all unused pins                      ; As output driving ground ;
; Base pin-out file on sameframe device        ; Off                      ;
+----------------------------------------------+--------------------------+


+------------------------------------+
; Operating Settings and Conditions  ;
+---------------------------+--------+
; Setting                   ; Value  ;
+---------------------------+--------+
; Nominal Core Voltage      ; 1.20 V ;
; Low Junction Temperature  ; 0 °C   ;
; High Junction Temperature ; 85 °C  ;
+---------------------------+--------+


+------------------------------------------------------------+
; Estimated Delay Added for Hold Timing                      ;
+-----------------+----------------------+-------------------+
; Source Clock(s) ; Destination Clock(s) ; Delay Added in ns ;
+-----------------+----------------------+-------------------+


+-----------------+
; Fitter Messages ;
+-----------------+
Info: *******************************************************************
Info: Running Quartus II Fitter
    Info: Version 9.1 Build 222 10/21/2009 SJ Full Version
    Info: Processing started: Mon May 28 14:21:59 2012
Info: Command: quartus_fit --read_settings_files=off --write_settings_files=off myArkanoid -c myArkanoid
Info: Parallel compilation is enabled and will use 2 of the 2 processors detected
Info: Selected device EP2C20F484C7 for design "myArkanoid"
Info: Low junction temperature is 0 degrees C
Info: High junction temperature is 85 degrees C
Info: Fitter is performing an Auto Fit compilation, which may decrease Fitter effort to reduce compilation time
Info: Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices
    Info: Device EP2C15AF484C7 is compatible
    Info: Device EP2C35F484C7 is compatible
    Info: Device EP2C50F484C7 is compatible
Info: Fitter converted 3 user pins into dedicated programming pins
    Info: Pin ~ASDO~ is reserved at location C4
    Info: Pin ~nCSO~ is reserved at location C3
    Info: Pin ~LVDS91p/nCEO~ is reserved at location W20
Info: Timing-driven compilation is using the Classic Timing Analyzer
Info: Timing requirements not specified -- quality metrics such as performance and power consumption may be sacrificed to reduce compilation time.
Info: Automatically promoted node ClockDivider:inst1|clk25MHz_ 
    Info: Automatically promoted destinations to use location or clock signal Global Clock
    Info: Following destination nodes may be non-global or may not use global or regional clocks
        Info: Destination node ClockDivider:inst1|clk25MHz_~0
Info: Starting register packing
Info: Finished register packing
    Extra Info: No registers were packed into other blocks
Info: Fitter preparation operations ending: elapsed time is 00:00:03
Info: Fitter placement preparation operations beginning
Info: Fitter placement preparation operations ending: elapsed time is 00:00:01
Info: Fitter placement operations beginning
Info: Fitter placement was successful
Info: Fitter placement operations ending: elapsed time is 00:00:03
Info: Estimated most critical path is register to register delay of 139.129 ns
    Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LAB_X32_Y11; Fanout = 36; REG Node = 'Arkanoid:inst|button2_state'
    Info: 2: + IC(0.779 ns) + CELL(0.544 ns) = 1.323 ns; Loc. = LAB_X33_Y13; Fanout = 73; COMB Node = 'Arkanoid:inst|platform2_position~4'
    Info: 3: + IC(0.740 ns) + CELL(0.521 ns) = 2.584 ns; Loc. = LAB_X33_Y15; Fanout = 63; COMB Node = 'Arkanoid:inst|platform2_position~5'
    Info: 4: + IC(1.073 ns) + CELL(0.495 ns) = 4.152 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~1'
    Info: 5: + IC(0.000 ns) + CELL(0.080 ns) = 4.232 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~3'
    Info: 6: + IC(0.000 ns) + CELL(0.080 ns) = 4.312 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~5'
    Info: 7: + IC(0.000 ns) + CELL(0.080 ns) = 4.392 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~7'
    Info: 8: + IC(0.000 ns) + CELL(0.080 ns) = 4.472 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~9'
    Info: 9: + IC(0.000 ns) + CELL(0.080 ns) = 4.552 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~11'
    Info: 10: + IC(0.000 ns) + CELL(0.080 ns) = 4.632 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~13'
    Info: 11: + IC(0.000 ns) + CELL(0.080 ns) = 4.712 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~15'
    Info: 12: + IC(0.000 ns) + CELL(0.080 ns) = 4.792 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~17'
    Info: 13: + IC(0.000 ns) + CELL(0.080 ns) = 4.872 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~19'
    Info: 14: + IC(0.000 ns) + CELL(0.080 ns) = 4.952 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~21'
    Info: 15: + IC(0.000 ns) + CELL(0.080 ns) = 5.032 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~23'
    Info: 16: + IC(0.000 ns) + CELL(0.080 ns) = 5.112 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~25'
    Info: 17: + IC(0.000 ns) + CELL(0.080 ns) = 5.192 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~27'
    Info: 18: + IC(0.000 ns) + CELL(0.080 ns) = 5.272 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~29'
    Info: 19: + IC(0.000 ns) + CELL(0.080 ns) = 5.352 ns; Loc. = LAB_X32_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~31'
    Info: 20: + IC(0.098 ns) + CELL(0.080 ns) = 5.530 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~33'
    Info: 21: + IC(0.000 ns) + CELL(0.080 ns) = 5.610 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~35'
    Info: 22: + IC(0.000 ns) + CELL(0.080 ns) = 5.690 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~37'
    Info: 23: + IC(0.000 ns) + CELL(0.080 ns) = 5.770 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~39'
    Info: 24: + IC(0.000 ns) + CELL(0.080 ns) = 5.850 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~41'
    Info: 25: + IC(0.000 ns) + CELL(0.080 ns) = 5.930 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~43'
    Info: 26: + IC(0.000 ns) + CELL(0.080 ns) = 6.010 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~45'
    Info: 27: + IC(0.000 ns) + CELL(0.080 ns) = 6.090 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~47'
    Info: 28: + IC(0.000 ns) + CELL(0.080 ns) = 6.170 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~49'
    Info: 29: + IC(0.000 ns) + CELL(0.080 ns) = 6.250 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~51'
    Info: 30: + IC(0.000 ns) + CELL(0.080 ns) = 6.330 ns; Loc. = LAB_X32_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|Add4~53'
    Info: 31: + IC(0.000 ns) + CELL(0.458 ns) = 6.788 ns; Loc. = LAB_X32_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|Add4~54'
    Info: 32: + IC(0.388 ns) + CELL(0.521 ns) = 7.697 ns; Loc. = LAB_X33_Y15; Fanout = 4; COMB Node = 'Arkanoid:inst|platform2_position~29'
    Info: 33: + IC(0.498 ns) + CELL(0.177 ns) = 8.372 ns; Loc. = LAB_X33_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan3~3'
    Info: 34: + IC(0.498 ns) + CELL(0.178 ns) = 9.048 ns; Loc. = LAB_X33_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan3~4'
    Info: 35: + IC(1.237 ns) + CELL(0.322 ns) = 10.607 ns; Loc. = LAB_X31_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|LessThan3~10'
    Info: 36: + IC(0.732 ns) + CELL(0.495 ns) = 11.834 ns; Loc. = LAB_X30_Y16; Fanout = 2; COMB Node = 'Arkanoid:inst|Add5~1'
    Info: 37: + IC(0.000 ns) + CELL(0.458 ns) = 12.292 ns; Loc. = LAB_X30_Y16; Fanout = 1; COMB Node = 'Arkanoid:inst|Add5~2'
    Info: 38: + IC(0.745 ns) + CELL(0.521 ns) = 13.558 ns; Loc. = LAB_X31_Y13; Fanout = 16; COMB Node = 'Arkanoid:inst|platform2_position~48'
    Info: 39: + IC(1.362 ns) + CELL(0.517 ns) = 15.437 ns; Loc. = LAB_X27_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|Add7~3'
    Info: 40: + IC(0.000 ns) + CELL(0.458 ns) = 15.895 ns; Loc. = LAB_X27_Y14; Fanout = 15; COMB Node = 'Arkanoid:inst|Add7~4'
    Info: 41: + IC(0.709 ns) + CELL(0.517 ns) = 17.121 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~5'
    Info: 42: + IC(0.000 ns) + CELL(0.080 ns) = 17.201 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~7'
    Info: 43: + IC(0.000 ns) + CELL(0.080 ns) = 17.281 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~9'
    Info: 44: + IC(0.000 ns) + CELL(0.080 ns) = 17.361 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~11'
    Info: 45: + IC(0.000 ns) + CELL(0.080 ns) = 17.441 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~13'
    Info: 46: + IC(0.000 ns) + CELL(0.080 ns) = 17.521 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~15'
    Info: 47: + IC(0.000 ns) + CELL(0.080 ns) = 17.601 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~17'
    Info: 48: + IC(0.000 ns) + CELL(0.080 ns) = 17.681 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~19'
    Info: 49: + IC(0.000 ns) + CELL(0.080 ns) = 17.761 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~21'
    Info: 50: + IC(0.000 ns) + CELL(0.080 ns) = 17.841 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~23'
    Info: 51: + IC(0.000 ns) + CELL(0.080 ns) = 17.921 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~25'
    Info: 52: + IC(0.000 ns) + CELL(0.080 ns) = 18.001 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~27'
    Info: 53: + IC(0.000 ns) + CELL(0.080 ns) = 18.081 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~29'
    Info: 54: + IC(0.000 ns) + CELL(0.080 ns) = 18.161 ns; Loc. = LAB_X26_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~31'
    Info: 55: + IC(0.098 ns) + CELL(0.080 ns) = 18.339 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~33'
    Info: 56: + IC(0.000 ns) + CELL(0.080 ns) = 18.419 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~35'
    Info: 57: + IC(0.000 ns) + CELL(0.080 ns) = 18.499 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~37'
    Info: 58: + IC(0.000 ns) + CELL(0.080 ns) = 18.579 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~39'
    Info: 59: + IC(0.000 ns) + CELL(0.080 ns) = 18.659 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~41'
    Info: 60: + IC(0.000 ns) + CELL(0.080 ns) = 18.739 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~43'
    Info: 61: + IC(0.000 ns) + CELL(0.080 ns) = 18.819 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~45'
    Info: 62: + IC(0.000 ns) + CELL(0.080 ns) = 18.899 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~47'
    Info: 63: + IC(0.000 ns) + CELL(0.080 ns) = 18.979 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~49'
    Info: 64: + IC(0.000 ns) + CELL(0.080 ns) = 19.059 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~51'
    Info: 65: + IC(0.000 ns) + CELL(0.080 ns) = 19.139 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~53'
    Info: 66: + IC(0.000 ns) + CELL(0.080 ns) = 19.219 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~55'
    Info: 67: + IC(0.000 ns) + CELL(0.080 ns) = 19.299 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~57'
    Info: 68: + IC(0.000 ns) + CELL(0.080 ns) = 19.379 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~59'
    Info: 69: + IC(0.000 ns) + CELL(0.080 ns) = 19.459 ns; Loc. = LAB_X26_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|LessThan139~61'
    Info: 70: + IC(0.000 ns) + CELL(0.458 ns) = 19.917 ns; Loc. = LAB_X26_Y13; Fanout = 3; COMB Node = 'Arkanoid:inst|LessThan139~62'
    Info: 71: + IC(0.763 ns) + CELL(0.521 ns) = 21.201 ns; Loc. = LAB_X26_Y11; Fanout = 9; COMB Node = 'Arkanoid:inst|always2~5'
    Info: 72: + IC(1.739 ns) + CELL(0.495 ns) = 23.435 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~1'
    Info: 73: + IC(0.000 ns) + CELL(0.080 ns) = 23.515 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~3'
    Info: 74: + IC(0.000 ns) + CELL(0.080 ns) = 23.595 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~5'
    Info: 75: + IC(0.000 ns) + CELL(0.080 ns) = 23.675 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~7'
    Info: 76: + IC(0.000 ns) + CELL(0.080 ns) = 23.755 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~9'
    Info: 77: + IC(0.000 ns) + CELL(0.080 ns) = 23.835 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~11'
    Info: 78: + IC(0.000 ns) + CELL(0.080 ns) = 23.915 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~13'
    Info: 79: + IC(0.000 ns) + CELL(0.080 ns) = 23.995 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~15'
    Info: 80: + IC(0.000 ns) + CELL(0.080 ns) = 24.075 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~17'
    Info: 81: + IC(0.000 ns) + CELL(0.080 ns) = 24.155 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~19'
    Info: 82: + IC(0.000 ns) + CELL(0.080 ns) = 24.235 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~21'
    Info: 83: + IC(0.000 ns) + CELL(0.080 ns) = 24.315 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~23'
    Info: 84: + IC(0.000 ns) + CELL(0.080 ns) = 24.395 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~25'
    Info: 85: + IC(0.000 ns) + CELL(0.080 ns) = 24.475 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~27'
    Info: 86: + IC(0.000 ns) + CELL(0.080 ns) = 24.555 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~29'
    Info: 87: + IC(0.000 ns) + CELL(0.080 ns) = 24.635 ns; Loc. = LAB_X13_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~31'
    Info: 88: + IC(0.098 ns) + CELL(0.080 ns) = 24.813 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~33'
    Info: 89: + IC(0.000 ns) + CELL(0.080 ns) = 24.893 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~35'
    Info: 90: + IC(0.000 ns) + CELL(0.080 ns) = 24.973 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~37'
    Info: 91: + IC(0.000 ns) + CELL(0.080 ns) = 25.053 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~39'
    Info: 92: + IC(0.000 ns) + CELL(0.080 ns) = 25.133 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~41'
    Info: 93: + IC(0.000 ns) + CELL(0.080 ns) = 25.213 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~43'
    Info: 94: + IC(0.000 ns) + CELL(0.080 ns) = 25.293 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~45'
    Info: 95: + IC(0.000 ns) + CELL(0.080 ns) = 25.373 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~47'
    Info: 96: + IC(0.000 ns) + CELL(0.080 ns) = 25.453 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~49'
    Info: 97: + IC(0.000 ns) + CELL(0.080 ns) = 25.533 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~51'
    Info: 98: + IC(0.000 ns) + CELL(0.080 ns) = 25.613 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~53'
    Info: 99: + IC(0.000 ns) + CELL(0.080 ns) = 25.693 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~55'
    Info: 100: + IC(0.000 ns) + CELL(0.080 ns) = 25.773 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~57'
    Info: 101: + IC(0.000 ns) + CELL(0.080 ns) = 25.853 ns; Loc. = LAB_X13_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Add9~59'
    Info: 102: + IC(0.000 ns) + CELL(0.080 ns) = 25.933 ns; Loc. = LAB_X13_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|Add9~61'
    Info: 103: + IC(0.000 ns) + CELL(0.458 ns) = 26.391 ns; Loc. = LAB_X13_Y10; Fanout = 3; COMB Node = 'Arkanoid:inst|Add9~63'
    Info: 104: + IC(0.745 ns) + CELL(0.521 ns) = 27.657 ns; Loc. = LAB_X12_Y13; Fanout = 4; COMB Node = 'Arkanoid:inst|lpm_divide:Mod0|lpm_divide_ako:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[0]~0'
    Info: 105: + IC(1.381 ns) + CELL(0.495 ns) = 29.533 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~1'
    Info: 106: + IC(0.000 ns) + CELL(0.080 ns) = 29.613 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~3'
    Info: 107: + IC(0.000 ns) + CELL(0.080 ns) = 29.693 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~5'
    Info: 108: + IC(0.000 ns) + CELL(0.080 ns) = 29.773 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~7'
    Info: 109: + IC(0.000 ns) + CELL(0.080 ns) = 29.853 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~9'
    Info: 110: + IC(0.000 ns) + CELL(0.080 ns) = 29.933 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~11'
    Info: 111: + IC(0.000 ns) + CELL(0.080 ns) = 30.013 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~13'
    Info: 112: + IC(0.000 ns) + CELL(0.080 ns) = 30.093 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~15'
    Info: 113: + IC(0.000 ns) + CELL(0.080 ns) = 30.173 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~17'
    Info: 114: + IC(0.000 ns) + CELL(0.080 ns) = 30.253 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~19'
    Info: 115: + IC(0.000 ns) + CELL(0.080 ns) = 30.333 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~21'
    Info: 116: + IC(0.000 ns) + CELL(0.080 ns) = 30.413 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~23'
    Info: 117: + IC(0.000 ns) + CELL(0.080 ns) = 30.493 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~25'
    Info: 118: + IC(0.000 ns) + CELL(0.080 ns) = 30.573 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~27'
    Info: 119: + IC(0.000 ns) + CELL(0.080 ns) = 30.653 ns; Loc. = LAB_X14_Y14; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~29'
    Info: 120: + IC(0.098 ns) + CELL(0.080 ns) = 30.831 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~31'
    Info: 121: + IC(0.000 ns) + CELL(0.080 ns) = 30.911 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~33'
    Info: 122: + IC(0.000 ns) + CELL(0.080 ns) = 30.991 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~35'
    Info: 123: + IC(0.000 ns) + CELL(0.080 ns) = 31.071 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~37'
    Info: 124: + IC(0.000 ns) + CELL(0.080 ns) = 31.151 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~39'
    Info: 125: + IC(0.000 ns) + CELL(0.080 ns) = 31.231 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~41'
    Info: 126: + IC(0.000 ns) + CELL(0.080 ns) = 31.311 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~43'
    Info: 127: + IC(0.000 ns) + CELL(0.080 ns) = 31.391 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~45'
    Info: 128: + IC(0.000 ns) + CELL(0.080 ns) = 31.471 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~47'
    Info: 129: + IC(0.000 ns) + CELL(0.080 ns) = 31.551 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~49'
    Info: 130: + IC(0.000 ns) + CELL(0.080 ns) = 31.631 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~51'
    Info: 131: + IC(0.000 ns) + CELL(0.080 ns) = 31.711 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~53'
    Info: 132: + IC(0.000 ns) + CELL(0.080 ns) = 31.791 ns; Loc. = LAB_X14_Y13; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~55'
    Info: 133: + IC(0.000 ns) + CELL(0.458 ns) = 32.249 ns; Loc. = LAB_X14_Y13; Fanout = 4; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|lpm_abs_0s9:my_abs_num|cs2a[1]~56'
    Info: 134: + IC(1.984 ns) + CELL(0.517 ns) = 34.750 ns; Loc. = LAB_X21_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_3_result_int[1]~1'
    Info: 135: + IC(0.000 ns) + CELL(0.080 ns) = 34.830 ns; Loc. = LAB_X21_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_3_result_int[2]~3'
    Info: 136: + IC(0.000 ns) + CELL(0.080 ns) = 34.910 ns; Loc. = LAB_X21_Y21; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_3_result_int[3]~5'
    Info: 137: + IC(0.000 ns) + CELL(0.458 ns) = 35.368 ns; Loc. = LAB_X21_Y21; Fanout = 14; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_3_result_int[4]~6'
    Info: 138: + IC(0.732 ns) + CELL(0.177 ns) = 36.277 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[18]~111'
    Info: 139: + IC(0.498 ns) + CELL(0.495 ns) = 37.270 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_4_result_int[1]~1'
    Info: 140: + IC(0.000 ns) + CELL(0.080 ns) = 37.350 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_4_result_int[2]~3'
    Info: 141: + IC(0.000 ns) + CELL(0.080 ns) = 37.430 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_4_result_int[3]~5'
    Info: 142: + IC(0.000 ns) + CELL(0.080 ns) = 37.510 ns; Loc. = LAB_X22_Y21; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_4_result_int[4]~7'
    Info: 143: + IC(0.000 ns) + CELL(0.458 ns) = 37.968 ns; Loc. = LAB_X22_Y21; Fanout = 17; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_4_result_int[5]~8'
    Info: 144: + IC(1.089 ns) + CELL(0.177 ns) = 39.234 ns; Loc. = LAB_X21_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[24]~121'
    Info: 145: + IC(1.089 ns) + CELL(0.495 ns) = 40.818 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_5_result_int[1]~1'
    Info: 146: + IC(0.000 ns) + CELL(0.080 ns) = 40.898 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_5_result_int[2]~3'
    Info: 147: + IC(0.000 ns) + CELL(0.080 ns) = 40.978 ns; Loc. = LAB_X22_Y21; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_5_result_int[3]~5'
    Info: 148: + IC(0.000 ns) + CELL(0.080 ns) = 41.058 ns; Loc. = LAB_X22_Y21; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_5_result_int[4]~7'
    Info: 149: + IC(0.000 ns) + CELL(0.080 ns) = 41.138 ns; Loc. = LAB_X22_Y21; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_5_result_int[5]~9'
    Info: 150: + IC(0.000 ns) + CELL(0.458 ns) = 41.596 ns; Loc. = LAB_X22_Y21; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_5_result_int[6]~10'
    Info: 151: + IC(1.397 ns) + CELL(0.177 ns) = 43.170 ns; Loc. = LAB_X20_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[30]~129'
    Info: 152: + IC(0.732 ns) + CELL(0.495 ns) = 44.397 ns; Loc. = LAB_X21_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_6_result_int[1]~1'
    Info: 153: + IC(0.000 ns) + CELL(0.080 ns) = 44.477 ns; Loc. = LAB_X21_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_6_result_int[2]~3'
    Info: 154: + IC(0.000 ns) + CELL(0.080 ns) = 44.557 ns; Loc. = LAB_X21_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_6_result_int[3]~5'
    Info: 155: + IC(0.000 ns) + CELL(0.080 ns) = 44.637 ns; Loc. = LAB_X21_Y17; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_6_result_int[4]~7'
    Info: 156: + IC(0.000 ns) + CELL(0.080 ns) = 44.717 ns; Loc. = LAB_X21_Y17; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_6_result_int[5]~9'
    Info: 157: + IC(0.000 ns) + CELL(0.458 ns) = 45.175 ns; Loc. = LAB_X21_Y17; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_6_result_int[6]~10'
    Info: 158: + IC(1.058 ns) + CELL(0.177 ns) = 46.410 ns; Loc. = LAB_X16_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[36]~137'
    Info: 159: + IC(1.039 ns) + CELL(0.495 ns) = 47.944 ns; Loc. = LAB_X20_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_7_result_int[1]~1'
    Info: 160: + IC(0.000 ns) + CELL(0.080 ns) = 48.024 ns; Loc. = LAB_X20_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_7_result_int[2]~3'
    Info: 161: + IC(0.000 ns) + CELL(0.080 ns) = 48.104 ns; Loc. = LAB_X20_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_7_result_int[3]~5'
    Info: 162: + IC(0.000 ns) + CELL(0.080 ns) = 48.184 ns; Loc. = LAB_X20_Y17; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_7_result_int[4]~7'
    Info: 163: + IC(0.000 ns) + CELL(0.080 ns) = 48.264 ns; Loc. = LAB_X20_Y17; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_7_result_int[5]~9'
    Info: 164: + IC(0.000 ns) + CELL(0.458 ns) = 48.722 ns; Loc. = LAB_X20_Y17; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_7_result_int[6]~10'
    Info: 165: + IC(1.396 ns) + CELL(0.177 ns) = 50.295 ns; Loc. = LAB_X16_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[42]~145'
    Info: 166: + IC(1.084 ns) + CELL(0.495 ns) = 51.874 ns; Loc. = LAB_X16_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_8_result_int[1]~1'
    Info: 167: + IC(0.000 ns) + CELL(0.080 ns) = 51.954 ns; Loc. = LAB_X16_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_8_result_int[2]~3'
    Info: 168: + IC(0.000 ns) + CELL(0.080 ns) = 52.034 ns; Loc. = LAB_X16_Y17; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_8_result_int[3]~5'
    Info: 169: + IC(0.000 ns) + CELL(0.080 ns) = 52.114 ns; Loc. = LAB_X16_Y17; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_8_result_int[4]~7'
    Info: 170: + IC(0.000 ns) + CELL(0.080 ns) = 52.194 ns; Loc. = LAB_X16_Y17; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_8_result_int[5]~9'
    Info: 171: + IC(0.000 ns) + CELL(0.458 ns) = 52.652 ns; Loc. = LAB_X16_Y17; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_8_result_int[6]~10'
    Info: 172: + IC(1.393 ns) + CELL(0.177 ns) = 54.222 ns; Loc. = LAB_X13_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[48]~153'
    Info: 173: + IC(1.039 ns) + CELL(0.495 ns) = 55.756 ns; Loc. = LAB_X16_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_9_result_int[1]~1'
    Info: 174: + IC(0.000 ns) + CELL(0.080 ns) = 55.836 ns; Loc. = LAB_X16_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_9_result_int[2]~3'
    Info: 175: + IC(0.000 ns) + CELL(0.080 ns) = 55.916 ns; Loc. = LAB_X16_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_9_result_int[3]~5'
    Info: 176: + IC(0.000 ns) + CELL(0.080 ns) = 55.996 ns; Loc. = LAB_X16_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_9_result_int[4]~7'
    Info: 177: + IC(0.000 ns) + CELL(0.080 ns) = 56.076 ns; Loc. = LAB_X16_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_9_result_int[5]~9'
    Info: 178: + IC(0.000 ns) + CELL(0.458 ns) = 56.534 ns; Loc. = LAB_X16_Y15; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_9_result_int[6]~10'
    Info: 179: + IC(0.940 ns) + CELL(0.319 ns) = 57.793 ns; Loc. = LAB_X16_Y17; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[57]~339'
    Info: 180: + IC(1.680 ns) + CELL(0.517 ns) = 59.990 ns; Loc. = LAB_X11_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_10_result_int[4]~7'
    Info: 181: + IC(0.000 ns) + CELL(0.080 ns) = 60.070 ns; Loc. = LAB_X11_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_10_result_int[5]~9'
    Info: 182: + IC(0.000 ns) + CELL(0.458 ns) = 60.528 ns; Loc. = LAB_X11_Y15; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_10_result_int[6]~10'
    Info: 183: + IC(0.914 ns) + CELL(0.319 ns) = 61.761 ns; Loc. = LAB_X16_Y15; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[63]~341'
    Info: 184: + IC(1.015 ns) + CELL(0.517 ns) = 63.293 ns; Loc. = LAB_X13_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_11_result_int[4]~7'
    Info: 185: + IC(0.000 ns) + CELL(0.080 ns) = 63.373 ns; Loc. = LAB_X13_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_11_result_int[5]~9'
    Info: 186: + IC(0.000 ns) + CELL(0.458 ns) = 63.831 ns; Loc. = LAB_X13_Y15; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_11_result_int[6]~10'
    Info: 187: + IC(1.040 ns) + CELL(0.177 ns) = 65.048 ns; Loc. = LAB_X9_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[66]~177'
    Info: 188: + IC(1.038 ns) + CELL(0.495 ns) = 66.581 ns; Loc. = LAB_X11_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_12_result_int[1]~1'
    Info: 189: + IC(0.000 ns) + CELL(0.080 ns) = 66.661 ns; Loc. = LAB_X11_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_12_result_int[2]~3'
    Info: 190: + IC(0.000 ns) + CELL(0.080 ns) = 66.741 ns; Loc. = LAB_X11_Y15; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_12_result_int[3]~5'
    Info: 191: + IC(0.000 ns) + CELL(0.080 ns) = 66.821 ns; Loc. = LAB_X11_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_12_result_int[4]~7'
    Info: 192: + IC(0.000 ns) + CELL(0.080 ns) = 66.901 ns; Loc. = LAB_X11_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_12_result_int[5]~9'
    Info: 193: + IC(0.000 ns) + CELL(0.458 ns) = 67.359 ns; Loc. = LAB_X11_Y15; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_12_result_int[6]~10'
    Info: 194: + IC(0.894 ns) + CELL(0.319 ns) = 68.572 ns; Loc. = LAB_X13_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[76]~344'
    Info: 195: + IC(1.016 ns) + CELL(0.517 ns) = 70.105 ns; Loc. = LAB_X10_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_13_result_int[5]~9'
    Info: 196: + IC(0.000 ns) + CELL(0.458 ns) = 70.563 ns; Loc. = LAB_X10_Y15; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_13_result_int[6]~10'
    Info: 197: + IC(1.038 ns) + CELL(0.177 ns) = 71.778 ns; Loc. = LAB_X12_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[82]~186'
    Info: 198: + IC(1.039 ns) + CELL(0.495 ns) = 73.312 ns; Loc. = LAB_X9_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_14_result_int[5]~9'
    Info: 199: + IC(0.000 ns) + CELL(0.458 ns) = 73.770 ns; Loc. = LAB_X9_Y15; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_14_result_int[6]~10'
    Info: 200: + IC(1.039 ns) + CELL(0.177 ns) = 74.986 ns; Loc. = LAB_X12_Y15; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[88]~194'
    Info: 201: + IC(1.382 ns) + CELL(0.495 ns) = 76.863 ns; Loc. = LAB_X9_Y14; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_15_result_int[5]~9'
    Info: 202: + IC(0.000 ns) + CELL(0.458 ns) = 77.321 ns; Loc. = LAB_X9_Y14; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_15_result_int[6]~10'
    Info: 203: + IC(1.089 ns) + CELL(0.177 ns) = 78.587 ns; Loc. = LAB_X9_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[90]~209'
    Info: 204: + IC(0.498 ns) + CELL(0.495 ns) = 79.580 ns; Loc. = LAB_X9_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_16_result_int[1]~1'
    Info: 205: + IC(0.000 ns) + CELL(0.080 ns) = 79.660 ns; Loc. = LAB_X9_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_16_result_int[2]~3'
    Info: 206: + IC(0.000 ns) + CELL(0.080 ns) = 79.740 ns; Loc. = LAB_X9_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_16_result_int[3]~5'
    Info: 207: + IC(0.000 ns) + CELL(0.080 ns) = 79.820 ns; Loc. = LAB_X9_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_16_result_int[4]~7'
    Info: 208: + IC(0.000 ns) + CELL(0.080 ns) = 79.900 ns; Loc. = LAB_X9_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_16_result_int[5]~9'
    Info: 209: + IC(0.000 ns) + CELL(0.458 ns) = 80.358 ns; Loc. = LAB_X9_Y10; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_16_result_int[6]~10'
    Info: 210: + IC(0.732 ns) + CELL(0.177 ns) = 81.267 ns; Loc. = LAB_X10_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[96]~217'
    Info: 211: + IC(0.498 ns) + CELL(0.495 ns) = 82.260 ns; Loc. = LAB_X10_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_17_result_int[1]~1'
    Info: 212: + IC(0.000 ns) + CELL(0.080 ns) = 82.340 ns; Loc. = LAB_X10_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_17_result_int[2]~3'
    Info: 213: + IC(0.000 ns) + CELL(0.080 ns) = 82.420 ns; Loc. = LAB_X10_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_17_result_int[3]~5'
    Info: 214: + IC(0.000 ns) + CELL(0.080 ns) = 82.500 ns; Loc. = LAB_X10_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_17_result_int[4]~7'
    Info: 215: + IC(0.000 ns) + CELL(0.080 ns) = 82.580 ns; Loc. = LAB_X10_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_17_result_int[5]~9'
    Info: 216: + IC(0.000 ns) + CELL(0.458 ns) = 83.038 ns; Loc. = LAB_X10_Y10; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_17_result_int[6]~10'
    Info: 217: + IC(1.084 ns) + CELL(0.177 ns) = 84.299 ns; Loc. = LAB_X9_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[102]~225'
    Info: 218: + IC(0.498 ns) + CELL(0.495 ns) = 85.292 ns; Loc. = LAB_X9_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_18_result_int[1]~1'
    Info: 219: + IC(0.000 ns) + CELL(0.080 ns) = 85.372 ns; Loc. = LAB_X9_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_18_result_int[2]~3'
    Info: 220: + IC(0.000 ns) + CELL(0.080 ns) = 85.452 ns; Loc. = LAB_X9_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_18_result_int[3]~5'
    Info: 221: + IC(0.000 ns) + CELL(0.080 ns) = 85.532 ns; Loc. = LAB_X9_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_18_result_int[4]~7'
    Info: 222: + IC(0.000 ns) + CELL(0.080 ns) = 85.612 ns; Loc. = LAB_X9_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_18_result_int[5]~9'
    Info: 223: + IC(0.000 ns) + CELL(0.458 ns) = 86.070 ns; Loc. = LAB_X9_Y12; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_18_result_int[6]~10'
    Info: 224: + IC(1.038 ns) + CELL(0.177 ns) = 87.285 ns; Loc. = LAB_X11_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[108]~233'
    Info: 225: + IC(0.498 ns) + CELL(0.495 ns) = 88.278 ns; Loc. = LAB_X11_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_19_result_int[1]~1'
    Info: 226: + IC(0.000 ns) + CELL(0.080 ns) = 88.358 ns; Loc. = LAB_X11_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_19_result_int[2]~3'
    Info: 227: + IC(0.000 ns) + CELL(0.080 ns) = 88.438 ns; Loc. = LAB_X11_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_19_result_int[3]~5'
    Info: 228: + IC(0.000 ns) + CELL(0.080 ns) = 88.518 ns; Loc. = LAB_X11_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_19_result_int[4]~7'
    Info: 229: + IC(0.000 ns) + CELL(0.080 ns) = 88.598 ns; Loc. = LAB_X11_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_19_result_int[5]~9'
    Info: 230: + IC(0.000 ns) + CELL(0.458 ns) = 89.056 ns; Loc. = LAB_X11_Y12; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_19_result_int[6]~10'
    Info: 231: + IC(1.089 ns) + CELL(0.177 ns) = 90.322 ns; Loc. = LAB_X10_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[114]~241'
    Info: 232: + IC(0.498 ns) + CELL(0.495 ns) = 91.315 ns; Loc. = LAB_X10_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_20_result_int[1]~1'
    Info: 233: + IC(0.000 ns) + CELL(0.080 ns) = 91.395 ns; Loc. = LAB_X10_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_20_result_int[2]~3'
    Info: 234: + IC(0.000 ns) + CELL(0.080 ns) = 91.475 ns; Loc. = LAB_X10_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_20_result_int[3]~5'
    Info: 235: + IC(0.000 ns) + CELL(0.080 ns) = 91.555 ns; Loc. = LAB_X10_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_20_result_int[4]~7'
    Info: 236: + IC(0.000 ns) + CELL(0.080 ns) = 91.635 ns; Loc. = LAB_X10_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_20_result_int[5]~9'
    Info: 237: + IC(0.000 ns) + CELL(0.458 ns) = 92.093 ns; Loc. = LAB_X10_Y9; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_20_result_int[6]~10'
    Info: 238: + IC(0.722 ns) + CELL(0.544 ns) = 93.359 ns; Loc. = LAB_X11_Y12; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[122]~244'
    Info: 239: + IC(1.066 ns) + CELL(0.517 ns) = 94.942 ns; Loc. = LAB_X11_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_21_result_int[3]~5'
    Info: 240: + IC(0.000 ns) + CELL(0.080 ns) = 95.022 ns; Loc. = LAB_X11_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_21_result_int[4]~7'
    Info: 241: + IC(0.000 ns) + CELL(0.080 ns) = 95.102 ns; Loc. = LAB_X11_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_21_result_int[5]~9'
    Info: 242: + IC(0.000 ns) + CELL(0.458 ns) = 95.560 ns; Loc. = LAB_X11_Y9; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_21_result_int[6]~10'
    Info: 243: + IC(0.365 ns) + CELL(0.544 ns) = 96.469 ns; Loc. = LAB_X10_Y9; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[128]~252'
    Info: 244: + IC(1.017 ns) + CELL(0.517 ns) = 98.003 ns; Loc. = LAB_X14_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_22_result_int[3]~5'
    Info: 245: + IC(0.000 ns) + CELL(0.080 ns) = 98.083 ns; Loc. = LAB_X14_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_22_result_int[4]~7'
    Info: 246: + IC(0.000 ns) + CELL(0.080 ns) = 98.163 ns; Loc. = LAB_X14_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_22_result_int[5]~9'
    Info: 247: + IC(0.000 ns) + CELL(0.458 ns) = 98.621 ns; Loc. = LAB_X14_Y9; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_22_result_int[6]~10'
    Info: 248: + IC(0.681 ns) + CELL(0.544 ns) = 99.846 ns; Loc. = LAB_X11_Y9; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[134]~260'
    Info: 249: + IC(1.017 ns) + CELL(0.517 ns) = 101.380 ns; Loc. = LAB_X15_Y9; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_23_result_int[3]~5'
    Info: 250: + IC(0.000 ns) + CELL(0.080 ns) = 101.460 ns; Loc. = LAB_X15_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_23_result_int[4]~7'
    Info: 251: + IC(0.000 ns) + CELL(0.080 ns) = 101.540 ns; Loc. = LAB_X15_Y9; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_23_result_int[5]~9'
    Info: 252: + IC(0.000 ns) + CELL(0.458 ns) = 101.998 ns; Loc. = LAB_X15_Y9; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_23_result_int[6]~10'
    Info: 253: + IC(0.375 ns) + CELL(0.544 ns) = 102.917 ns; Loc. = LAB_X14_Y9; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[140]~268'
    Info: 254: + IC(1.060 ns) + CELL(0.517 ns) = 104.494 ns; Loc. = LAB_X15_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_24_result_int[3]~5'
    Info: 255: + IC(0.000 ns) + CELL(0.080 ns) = 104.574 ns; Loc. = LAB_X15_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_24_result_int[4]~7'
    Info: 256: + IC(0.000 ns) + CELL(0.080 ns) = 104.654 ns; Loc. = LAB_X15_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_24_result_int[5]~9'
    Info: 257: + IC(0.000 ns) + CELL(0.458 ns) = 105.112 ns; Loc. = LAB_X15_Y10; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_24_result_int[6]~10'
    Info: 258: + IC(0.716 ns) + CELL(0.544 ns) = 106.372 ns; Loc. = LAB_X15_Y9; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[146]~276'
    Info: 259: + IC(1.060 ns) + CELL(0.517 ns) = 107.949 ns; Loc. = LAB_X16_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_25_result_int[3]~5'
    Info: 260: + IC(0.000 ns) + CELL(0.080 ns) = 108.029 ns; Loc. = LAB_X16_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_25_result_int[4]~7'
    Info: 261: + IC(0.000 ns) + CELL(0.080 ns) = 108.109 ns; Loc. = LAB_X16_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_25_result_int[5]~9'
    Info: 262: + IC(0.000 ns) + CELL(0.458 ns) = 108.567 ns; Loc. = LAB_X16_Y10; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_25_result_int[6]~10'
    Info: 263: + IC(0.365 ns) + CELL(0.544 ns) = 109.476 ns; Loc. = LAB_X15_Y10; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[152]~284'
    Info: 264: + IC(1.060 ns) + CELL(0.517 ns) = 111.053 ns; Loc. = LAB_X16_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_26_result_int[3]~5'
    Info: 265: + IC(0.000 ns) + CELL(0.080 ns) = 111.133 ns; Loc. = LAB_X16_Y11; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_26_result_int[4]~7'
    Info: 266: + IC(0.000 ns) + CELL(0.080 ns) = 111.213 ns; Loc. = LAB_X16_Y11; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_26_result_int[5]~9'
    Info: 267: + IC(0.000 ns) + CELL(0.458 ns) = 111.671 ns; Loc. = LAB_X16_Y11; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_26_result_int[6]~10'
    Info: 268: + IC(0.706 ns) + CELL(0.544 ns) = 112.921 ns; Loc. = LAB_X16_Y10; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[158]~292'
    Info: 269: + IC(1.050 ns) + CELL(0.517 ns) = 114.488 ns; Loc. = LAB_X15_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_27_result_int[3]~5'
    Info: 270: + IC(0.000 ns) + CELL(0.080 ns) = 114.568 ns; Loc. = LAB_X15_Y11; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_27_result_int[4]~7'
    Info: 271: + IC(0.000 ns) + CELL(0.080 ns) = 114.648 ns; Loc. = LAB_X15_Y11; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_27_result_int[5]~9'
    Info: 272: + IC(0.000 ns) + CELL(0.458 ns) = 115.106 ns; Loc. = LAB_X15_Y11; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_27_result_int[6]~10'
    Info: 273: + IC(0.375 ns) + CELL(0.544 ns) = 116.025 ns; Loc. = LAB_X16_Y11; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[164]~300'
    Info: 274: + IC(1.358 ns) + CELL(0.517 ns) = 117.900 ns; Loc. = LAB_X14_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_28_result_int[3]~5'
    Info: 275: + IC(0.000 ns) + CELL(0.080 ns) = 117.980 ns; Loc. = LAB_X14_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_28_result_int[4]~7'
    Info: 276: + IC(0.000 ns) + CELL(0.080 ns) = 118.060 ns; Loc. = LAB_X14_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_28_result_int[5]~9'
    Info: 277: + IC(0.000 ns) + CELL(0.458 ns) = 118.518 ns; Loc. = LAB_X14_Y12; Fanout = 16; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_28_result_int[6]~10'
    Info: 278: + IC(0.716 ns) + CELL(0.544 ns) = 119.778 ns; Loc. = LAB_X15_Y11; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[170]~308'
    Info: 279: + IC(1.060 ns) + CELL(0.517 ns) = 121.355 ns; Loc. = LAB_X15_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_29_result_int[3]~5'
    Info: 280: + IC(0.000 ns) + CELL(0.080 ns) = 121.435 ns; Loc. = LAB_X15_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_29_result_int[4]~7'
    Info: 281: + IC(0.000 ns) + CELL(0.080 ns) = 121.515 ns; Loc. = LAB_X15_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_29_result_int[5]~9'
    Info: 282: + IC(0.000 ns) + CELL(0.458 ns) = 121.973 ns; Loc. = LAB_X15_Y12; Fanout = 17; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_29_result_int[6]~10'
    Info: 283: + IC(0.375 ns) + CELL(0.544 ns) = 122.892 ns; Loc. = LAB_X14_Y12; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[176]~316'
    Info: 284: + IC(1.024 ns) + CELL(0.517 ns) = 124.433 ns; Loc. = LAB_X16_Y12; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_30_result_int[3]~5'
    Info: 285: + IC(0.000 ns) + CELL(0.080 ns) = 124.513 ns; Loc. = LAB_X16_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_30_result_int[4]~7'
    Info: 286: + IC(0.000 ns) + CELL(0.080 ns) = 124.593 ns; Loc. = LAB_X16_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_30_result_int[5]~9'
    Info: 287: + IC(0.000 ns) + CELL(0.458 ns) = 125.051 ns; Loc. = LAB_X16_Y12; Fanout = 13; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_30_result_int[6]~10'
    Info: 288: + IC(0.365 ns) + CELL(0.544 ns) = 125.960 ns; Loc. = LAB_X15_Y12; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|StageOut[182]~324'
    Info: 289: + IC(1.060 ns) + CELL(0.517 ns) = 127.537 ns; Loc. = LAB_X16_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_31_result_int[3]~5'
    Info: 290: + IC(0.000 ns) + CELL(0.080 ns) = 127.617 ns; Loc. = LAB_X16_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_31_result_int[4]~7'
    Info: 291: + IC(0.000 ns) + CELL(0.080 ns) = 127.697 ns; Loc. = LAB_X16_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_31_result_int[5]~9'
    Info: 292: + IC(0.000 ns) + CELL(0.458 ns) = 128.155 ns; Loc. = LAB_X16_Y13; Fanout = 3; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|alt_u_div_k2f:divider|add_sub_31_result_int[6]~10'
    Info: 293: + IC(1.369 ns) + CELL(0.517 ns) = 130.041 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~1'
    Info: 294: + IC(0.000 ns) + CELL(0.080 ns) = 130.121 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~3'
    Info: 295: + IC(0.000 ns) + CELL(0.080 ns) = 130.201 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~5'
    Info: 296: + IC(0.000 ns) + CELL(0.080 ns) = 130.281 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~7'
    Info: 297: + IC(0.000 ns) + CELL(0.080 ns) = 130.361 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~9'
    Info: 298: + IC(0.000 ns) + CELL(0.080 ns) = 130.441 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~11'
    Info: 299: + IC(0.000 ns) + CELL(0.080 ns) = 130.521 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~13'
    Info: 300: + IC(0.000 ns) + CELL(0.080 ns) = 130.601 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~15'
    Info: 301: + IC(0.000 ns) + CELL(0.080 ns) = 130.681 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~17'
    Info: 302: + IC(0.000 ns) + CELL(0.080 ns) = 130.761 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~19'
    Info: 303: + IC(0.000 ns) + CELL(0.080 ns) = 130.841 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~21'
    Info: 304: + IC(0.000 ns) + CELL(0.080 ns) = 130.921 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~23'
    Info: 305: + IC(0.000 ns) + CELL(0.080 ns) = 131.001 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~25'
    Info: 306: + IC(0.000 ns) + CELL(0.080 ns) = 131.081 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~27'
    Info: 307: + IC(0.000 ns) + CELL(0.080 ns) = 131.161 ns; Loc. = LAB_X18_Y11; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~29'
    Info: 308: + IC(0.098 ns) + CELL(0.080 ns) = 131.339 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~31'
    Info: 309: + IC(0.000 ns) + CELL(0.080 ns) = 131.419 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~33'
    Info: 310: + IC(0.000 ns) + CELL(0.080 ns) = 131.499 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~35'
    Info: 311: + IC(0.000 ns) + CELL(0.080 ns) = 131.579 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~37'
    Info: 312: + IC(0.000 ns) + CELL(0.080 ns) = 131.659 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~39'
    Info: 313: + IC(0.000 ns) + CELL(0.080 ns) = 131.739 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~41'
    Info: 314: + IC(0.000 ns) + CELL(0.080 ns) = 131.819 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~43'
    Info: 315: + IC(0.000 ns) + CELL(0.080 ns) = 131.899 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~45'
    Info: 316: + IC(0.000 ns) + CELL(0.080 ns) = 131.979 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~47'
    Info: 317: + IC(0.000 ns) + CELL(0.080 ns) = 132.059 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~49'
    Info: 318: + IC(0.000 ns) + CELL(0.080 ns) = 132.139 ns; Loc. = LAB_X18_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~51'
    Info: 319: + IC(0.000 ns) + CELL(0.458 ns) = 132.597 ns; Loc. = LAB_X18_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|lpm_divide:Div0|lpm_divide_7so:auto_generated|abs_divider_kbg:divider|op_1~52'
    Info: 320: + IC(0.732 ns) + CELL(0.178 ns) = 133.507 ns; Loc. = LAB_X19_Y10; Fanout = 2; COMB Node = 'Arkanoid:inst|Equal6~2'
    Info: 321: + IC(0.131 ns) + CELL(0.545 ns) = 134.183 ns; Loc. = LAB_X19_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|Equal6~3'
    Info: 322: + IC(0.354 ns) + CELL(0.322 ns) = 134.859 ns; Loc. = LAB_X19_Y10; Fanout = 1; COMB Node = 'Arkanoid:inst|Equal6~7'
    Info: 323: + IC(1.034 ns) + CELL(0.544 ns) = 136.437 ns; Loc. = LAB_X15_Y13; Fanout = 5; COMB Node = 'Arkanoid:inst|Equal6~24'
    Info: 324: + IC(0.131 ns) + CELL(0.545 ns) = 137.113 ns; Loc. = LAB_X15_Y13; Fanout = 4; COMB Node = 'Arkanoid:inst|WideNor0~4'
    Info: 325: + IC(0.131 ns) + CELL(0.545 ns) = 137.789 ns; Loc. = LAB_X15_Y13; Fanout = 3; COMB Node = 'Arkanoid:inst|WideOr0~0'
    Info: 326: + IC(0.723 ns) + CELL(0.521 ns) = 139.033 ns; Loc. = LAB_X10_Y13; Fanout = 1; COMB Node = 'Arkanoid:inst|high~8'
    Info: 327: + IC(0.000 ns) + CELL(0.096 ns) = 139.129 ns; Loc. = LAB_X10_Y13; Fanout = 1; REG Node = 'Arkanoid:inst|hex3_[5]'
    Info: Total cell delay = 67.965 ns ( 48.85 % )
    Info: Total interconnect delay = 71.164 ns ( 51.15 % )
Info: Fitter routing operations beginning
Info: Average interconnect usage is 13% of the available device resources
    Info: Peak interconnect usage is 26% of the available device resources in the region that extends from location X25_Y14 to location X37_Y27
Info: Fitter routing operations ending: elapsed time is 00:00:08
Info: The Fitter performed an Auto Fit compilation.  Optimizations were skipped to reduce compilation time.
    Info: Optimizations that may affect the design's routability were skipped
    Info: Optimizations that may affect the design's timing were skipped
Info: Started post-fitting delay annotation
Warning: Found 50 output pins without output pin load capacitance assignment
    Info: Pin "h_sync" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "v_sync" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "blue[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "blue[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "blue[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "blue[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "green[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "green[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "green[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "green[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[6]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[5]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[4]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex0[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[6]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[5]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[4]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex1[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[6]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[5]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[4]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex2[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[6]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[5]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[4]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "hex3[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[7]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[6]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[5]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[4]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "led[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "red[3]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "red[2]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "red[1]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
    Info: Pin "red[0]" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis
Info: Delay annotation completed successfully
Warning: The Reserve All Unused Pins setting has not been specified, and will default to 'As output driving ground'.
Info: Generated suppressed messages file G:/Verilog/Arkanoid2PDE1/myArkanoid.fit.smsg
Info: Quartus II Fitter was successful. 0 errors, 2 warnings
    Info: Peak virtual memory: 266 megabytes
    Info: Processing ended: Mon May 28 14:22:27 2012
    Info: Elapsed time: 00:00:28
    Info: Total CPU time (on all processors): 00:00:31


+----------------------------+
; Fitter Suppressed Messages ;
+----------------------------+
The suppressed messages can be found in G:/Verilog/Arkanoid2PDE1/myArkanoid.fit.smsg.


