/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2009 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 16 16 168 240)
	(text "Arkanoid" (rect 5 0 47 12)(font "Arial" ))
	(text "inst" (rect 8 208 25 220)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "clk25MHz" (rect 0 0 47 12)(font "Arial" ))
		(text "clk25MHz" (rect 21 27 68 39)(font "Arial" ))
		(line (pt 0 32)(pt 16 32)(line_width 1))
	)
	(port
		(pt 0 48)
		(input)
		(text "button1" (rect 0 0 36 12)(font "Arial" ))
		(text "button1" (rect 21 43 57 55)(font "Arial" ))
		(line (pt 0 48)(pt 16 48)(line_width 1))
	)
	(port
		(pt 0 64)
		(input)
		(text "button2" (rect 0 0 36 12)(font "Arial" ))
		(text "button2" (rect 21 59 57 71)(font "Arial" ))
		(line (pt 0 64)(pt 16 64)(line_width 1))
	)
	(port
		(pt 0 80)
		(input)
		(text "button3" (rect 0 0 36 12)(font "Arial" ))
		(text "button3" (rect 21 75 57 87)(font "Arial" ))
		(line (pt 0 80)(pt 16 80)(line_width 1))
	)
	(port
		(pt 0 96)
		(input)
		(text "button4" (rect 0 0 36 12)(font "Arial" ))
		(text "button4" (rect 21 91 57 103)(font "Arial" ))
		(line (pt 0 96)(pt 16 96)(line_width 1))
	)
	(port
		(pt 152 32)
		(output)
		(text "h_sync" (rect 0 0 36 12)(font "Arial" ))
		(text "h_sync" (rect 95 27 131 39)(font "Arial" ))
		(line (pt 152 32)(pt 136 32)(line_width 1))
	)
	(port
		(pt 152 48)
		(output)
		(text "v_sync" (rect 0 0 37 12)(font "Arial" ))
		(text "v_sync" (rect 94 43 131 55)(font "Arial" ))
		(line (pt 152 48)(pt 136 48)(line_width 1))
	)
	(port
		(pt 152 64)
		(output)
		(text "red[3..0]" (rect 0 0 41 12)(font "Arial" ))
		(text "red[3..0]" (rect 90 59 131 71)(font "Arial" ))
		(line (pt 152 64)(pt 136 64)(line_width 3))
	)
	(port
		(pt 152 80)
		(output)
		(text "green[3..0]" (rect 0 0 53 12)(font "Arial" ))
		(text "green[3..0]" (rect 78 75 131 87)(font "Arial" ))
		(line (pt 152 80)(pt 136 80)(line_width 3))
	)
	(port
		(pt 152 96)
		(output)
		(text "blue[3..0]" (rect 0 0 46 12)(font "Arial" ))
		(text "blue[3..0]" (rect 85 91 131 103)(font "Arial" ))
		(line (pt 152 96)(pt 136 96)(line_width 3))
	)
	(port
		(pt 152 112)
		(output)
		(text "hex0[6..0]" (rect 0 0 49 12)(font "Arial" ))
		(text "hex0[6..0]" (rect 82 107 131 119)(font "Arial" ))
		(line (pt 152 112)(pt 136 112)(line_width 3))
	)
	(port
		(pt 152 128)
		(output)
		(text "hex1[6..0]" (rect 0 0 49 12)(font "Arial" ))
		(text "hex1[6..0]" (rect 82 123 131 135)(font "Arial" ))
		(line (pt 152 128)(pt 136 128)(line_width 3))
	)
	(port
		(pt 152 144)
		(output)
		(text "hex2[6..0]" (rect 0 0 49 12)(font "Arial" ))
		(text "hex2[6..0]" (rect 82 139 131 151)(font "Arial" ))
		(line (pt 152 144)(pt 136 144)(line_width 3))
	)
	(port
		(pt 152 160)
		(output)
		(text "hex3[6..0]" (rect 0 0 49 12)(font "Arial" ))
		(text "hex3[6..0]" (rect 82 155 131 167)(font "Arial" ))
		(line (pt 152 160)(pt 136 160)(line_width 3))
	)
	(port
		(pt 152 176)
		(output)
		(text "led[7..0]" (rect 0 0 40 12)(font "Arial" ))
		(text "led[7..0]" (rect 91 171 131 183)(font "Arial" ))
		(line (pt 152 176)(pt 136 176)(line_width 3))
	)
	(parameter
		"CELL_SIZE"
		"20"
		""
		(type "PARAMETER_SIGNED_DEC")	)
	(parameter
		"BALL_SIZE"
		"1"
		""
		(type "PARAMETER_SIGNED_DEC")	)
	(parameter
		"BALL_SPEED"
		"1"
		""
		(type "PARAMETER_SIGNED_DEC")	)
	(parameter
		"PLATFORM_WIDTH"
		"7"
		""
		(type "PARAMETER_SIGNED_DEC")	)
	(parameter
		"BK_COLOR_R"
		"1111"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"BK_COLOR_G"
		"0000"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"BK_COLOR_B"
		"0000"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"STABLE_COLOR_R"
		"0011"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"STABLE_COLOR_G"
		"1100"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"STABLE_COLOR_B"
		"0110"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"BALL_COLOR_R"
		"0000"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"BALL_COLOR_G"
		"0000"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"BALL_COLOR_B"
		"1111"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"PLATFORM_COLOR_R"
		"1111"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"PLATFORM_COLOR_G"
		"0000"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(parameter
		"PLATFORM_COLOR_B"
		"0000"
		""
		(type "PARAMETER_UNSIGNED_BIN")	)
	(drawing
		(rectangle (rect 16 16 136 208)(line_width 1))
	)
	(annotation_block (parameter)(rect 168 -64 268 16))
)
